Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	178 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6119575 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	526950  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Stable, Present (stbank) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db1.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Very dark brown (10YR2/3-Moist); ; Fine sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Slightly 
	plastic; Moderately sticky; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Clear, Smooth 
	change to - 
	A2	0.15 - 0.28 m	Brown (10YR5/3-Moist); Very pale brown (10YR7/3-Dry); Mottles, 2-10% , Faint; Coarse sandy 
	clay loam; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moderately 
	moist; Slightly plastic; Moderately sticky; Field pH 6 (Raupach); Common, fine (1-2mm) roots; 
	Clear, Smooth change to - 
	B	0.28 - 0.9 m	Very dark brown (10YR2/3-Moist); Mottles, 2-10% , Faint; Medium clay; Strong grade of structure, 
	20-50 mm, Angular blocky; 50-100 mm, Columnar; Smooth-ped fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Moist; Moderately plastic; Very sticky; Common cutans, 10-
	50% of ped faces or walls coated, faint; Field pH 7.5 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	A2	High silt content.                                                                                                                  
	                                                                    
	Observation Notes
	River bank exposure                                                                                                                                                                            
	         
	Site Notes
	30M IN FENCE, W RIVER BANK CLIFF      

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile