Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW150	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	210 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6119625 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	524100  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgc	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (sheet) Partial, Moderate (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Kandosol Medium Slightly gravelly Sandy  	Principal Profile Form:	Gn2.12
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Medium sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Slightly plastic; 
	Moderately sticky; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments;
	 Field pH 6 (Raupach); Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B	0.1 - 0.45 m	Yellowish red (5YR4/6-Moist); ; Coarse sandy light clay; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Dry; Moderately plastic; Very sticky; 0-2%, fine gravelly, 2-
	6mm, subrounded, dispersed, Quartz, coarse fragments; Few (2 - 10 %), Ferromanganiferous, 
	Fine (0 - 2 mm), Nodules, strong, segregations;Few (2 - 10 %), Ferromanganiferous, Medium (2 -
	6 mm), Nodules, strong, segregations;Field pH 6.5 (Raupach); Common, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	BC	0.45 - 1 m	Dark yellowish brown (10YR4/6-Moist); Mottles, 2-10% , Distinct; Mottles, 2-10% , Faint; Medium 
	sandy light medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; 
	Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Moderately plastic; Very sticky; 2-
	10%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 7 (Raupach); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	A	Some may have been removed by previous  sheet erosion.                                                 
	                                                                                                 
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW150	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW150	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile