Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	188 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6112750 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	545350  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Moderate (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Db1.33
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (10YR3/3-Moist); ; Clay loam; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; Smooth-ped fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; 
	Moderately plastic; Very sticky; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Clear, Smooth
	 change to - 
	A2	0.15 - 0.25 m	Brown (10YR4/3-Moist); Very pale brown (10YR7/3-Dry); ; Silty clay loam; Weak grade of 
	structure, 50-100 mm, Subangular blocky; Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per
	 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Firm consistence; Slightly plastic; Very sticky; Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Clear, Smooth change to - 
	B2	0.25 - 0.55 m	Dark brown (10YR3/3-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; 100-200 mm, Lenticular; Rough-ped fabric; Fine, (0 - 5) mm crack; Common 
	(1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Very firm consistence; Moderately plastic; Very sticky; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 7.5 (Raupach); 
	Common, fine (1-2mm) roots; Clear, Wavy change to - 
	C	0.55 - 1.1 m	Dark greyish brown (2.5Y4/2-Moist); Mottles, 0-2% , Faint; Medium clay; Strong grade of 
	structure, 5-10 mm, Polyhedral; Smooth-ped fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2)
	 Very fine (0.075-1mm) macropores, Dry; Very firm consistence; Very plastic; Very sticky; 0-2%, 
	fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; Few cutans, <10% of ped faces
	 or walls coated, faint; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, 
	segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 9.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	40M IN FENCE, S SIDE OF GULLY         

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW171	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile