Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	289 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6102175 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	540550  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ou	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	15 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Chromosol Thin Gravelly Sandy  Very shallow	Principal Profile Form:	Dr2.21
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subangular, Sandstone; No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Loam; Massive grade of structure; Earthy fabric; Common (1-5 per
	 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Weak consistence; Slightly plastic; Slightly sticky; 10-20%, fine gravelly, 2-
	6mm, subangular, dispersed, Sandstone, coarse fragments; Field pH 5.5 (Raupach); Many, fine 
	(1-2mm) roots; Gradual, Smooth change to - 
	A2	0.1 - 0.25 m	Reddish brown (5YR4/4-Moist); Light reddish brown (5YR6/4-Dry); ; Fine sandy clay loam; 
	Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Slightly 
	plastic; Moderately sticky; 20-50%, fine gravelly, 2-6mm, subangular, dispersed, Sandstone, 
	coarse fragments; Field pH 5.5 (Raupach); Common, fine (1-2mm) roots; Clear, Smooth change 
	to - 
	B	0.25 - 0.45 m	Yellowish red (5YR4/8-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Strong 
	consistence; Moderately plastic; Very sticky; 2-10%, fine gravelly, 2-6mm, subangular, 
	dispersed, Sandstone, coarse fragments; Field pH 6 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW178	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile