Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW180	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	218 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6105825 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	532300  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR4/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Common (1-5 per
	 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, 
	Dry; Weak consistence; Moderately plastic; Slightly sticky; Field pH 5.5 (Raupach); Common, 
	fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.08 - 0.5 m	Light brown (7.5YR6/4-Moist); Pinkish grey (7.5YR7/3-Dry); Mottles, 0-2% , Distinct; Silty clay 
	loam; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm 
	consistence; Moderately plastic; Moderately sticky; Common (10 - 20 %), Ferromanganiferous, 
	Fine (0 - 2 mm), Nodules, strong, segregations;Common (10 - 20 %), Ferromanganiferous, 
	Medium (2 -6 mm), Nodules, strong, segregations;Field pH 5.5 (Raupach); Common, fine (1-
	2mm) roots; Clear change to - 
	B	0.5 - 0.75 m	Yellowish brown (10YR5/4-Moist); Mottles, 10-20% , Faint; Light clay; Moderate grade of 
	structure, 2-5 mm, Polyhedral; Rough-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Dry; Very firm consistence; Moderately plastic; Very sticky; Few (2 - 10 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 7 (Raupach); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	B	Dry compact, difficult for augering.                                                                                       
	                                                                             
	Observation Notes
	Pit to 30cm, ager to 75cm.                                                                                                                                                                 
	             
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW180	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW180	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile