Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	248 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6108100 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	525475  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ou	Substrate Material:	Shale 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	7 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hyperbasic Red Chromosol Thick Gravelly Loamy  	Principal Profile Form:	Dr2.41
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; Field pH 5.5 
	(Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.15 - 0.28 m	Yellowish red (5YR5/6-Moist); Pink (5YR7/4-Dry); ; Fine sandy clay loam; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 
	per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Slightly plastic; Moderately 
	sticky; Field pH 5 (Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B2	0.28 - 0.45 m	Red (2.5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, Polyhedral; Rough-
	ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine
	 (1-2mm) macropores, Dry; Very firm consistence; Very plastic; Very sticky; 10-20%, fine 
	gravelly, 2-6mm, subangular platy, dispersed, Shale, coarse fragments; Field pH 5.5 (Raupach);
	 Common, fine (1-2mm) roots; Gradual change to - 
	BC	0.45 - 0.75 m	Yellowish red (5YR5/8-Moist); Substrate influence, 10-20% , Distinct; Medium clay; Moderate 
	grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Dry; Moderately plastic; Very sticky; 
	20-50%, fine gravelly, 2-6mm, subangular platy, stratified, Shale, coarse fragments; Field pH 5.5
	 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile