Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW197	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	186 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6111425 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	538600  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Crusty Grey Vertosol     	Principal Profile Form:	Ug5.2
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Very dark brown (10YR2/3-Moist); Mottles, 10-20% , Distinct; Light clay; Moderate grade of 
	structure, 20-50 mm, Polyhedral; 100-200 mm, Prismatic; Smooth-ped fabric; Fine, (0 - 5) mm 
	crack; Medium, (5 - 10) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry;
	 Very firm consistence; Moderately plastic; Very sticky; Very few (0 - 2 %), Ferromanganiferous, 
	Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), Ferromanganiferous, Medium 
	(2 -6 mm), Nodules, strong, segregations;Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; 
	Clear, Smooth change to - 
	B	0.1 - 0.8 m	Dark grey (2.5Y4/1-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, Polyhedral; 100-
	200 mm, Lenticular; Smooth-ped fabric; Fine, (0 - 5) mm crack; Medium, (5 - 10) mm crack; Few 
	(<1 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very firm consistence; Very plastic; 
	Very sticky; Few cutans, <10% of ped faces or walls coated, faint; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Calcareous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), Calcareous, 
	Medium (2 -6 mm), Nodules, strong, segregations;Field pH 9 (Raupach); Common, fine (1-2mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Artificial drainage line exposure.      At slightly lower part of the alluvial  plain.                                                                                
	                                  
	Site Notes
	80M IN FENCE, N BANK                  

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW197	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW197	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile