Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	292 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6083900 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	529050  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/2-Moist); ; Clay loam; Moderate grade of structure, 10-20 mm, Subangular blocky;
	 Rough-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Moderately plastic; Moderately 
	sticky; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.1 - 0.2 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/2-Dry); Biological mixing, 0-2% , Distinct; 
	Sandy loam; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm 
	consistence; Slightly plastic; Moderately sticky; Field pH 5.5 (Raupach); Common, fine (1-2mm) 
	roots; Gradual, Smooth change to - 
	B	0.2 - 0.45 m	Yellowish brown (10YR5/4-Moist); Mottles, 10-20% , Distinct; Light medium clay; Moderate 
	grade of structure, 50-100 mm, Angular blocky; 100-200 mm, Prismatic; Smooth-ped fabric; Few
	 (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Strong consistence; Moderately plastic; Very sticky; Field pH 5.5 (Raupach); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	40M W GATE, N OF RIDE                 

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW201	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile