Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	390 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6083500 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	532675  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Ou	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	5 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Orthic Rudosol     	Principal Profile Form:	Um1.23
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.22 m	Dark brown (7.5YR3/2-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Rough-ped fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common 
	(1-5 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 100mm2) Medium (2-5mm) 
	macropores, Dry; Weak consistence; Moderately plastic; Moderately sticky; 0-2%, medium 
	gravelly, 6-20mm, subangular, dispersed, coarse fragments; Field pH 5.5 (Raupach); Many, fine 
	(1-2mm) roots; Gradual, Smooth change to - 
	C1	0.22 - 0.42 m	Dark brown (7.5YR3/3-Moist); ; Clay loam; Weak grade of structure, 5-10 mm, Subangular blocky;
	 Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Few (<1 per 100mm2) Medium (2-5mm) macropores, Dry; 
	Weak consistence; Moderately plastic; Very sticky; 0-2%, medium gravelly, 6-20mm, 
	subangular, dispersed, coarse fragments; Field pH 5 (Raupach); Common, fine (1-2mm) roots; 
	Gradual change to - 
	C2	0.42 - 0.7 m	Dark brown (7.5YR3/2-Moist); Mottles, 2-10% , Faint; Clay loam; Massive grade of structure; 
	Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Moderately plastic; Moderately 
	sticky; Field pH 5 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	A1	Charcoals.                                                                                                                            
	                                                                  
	C1	Charcoals.                                                                                                                            
	                                                                  
	C2	Rich in charcoals.                                                                                                                
	                                                                      
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.22	4.1B	0.07A	1.1J	1.4	0.6	0.6	1.2L	5.5I	10.91
	0.22 - 0.42	4.3B	0.04A	0.2J	2.5	0.3	0.8	0.6L	7.1I	11.27
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.22	3.96A	4D	1	5F	49	32	13
	0.22 - 0.42	1.83A	1D	6F	38	34	22
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.22	0.6B	0.13B
	0.22 - 0.42	0.54B	0.13B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW202	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_GRAV	Gravel (%)
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate