Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	331 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6072550 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	537675  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	2 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.2 m	Brown (7.5YR4/3-Moist); ; Fine sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Slightly plastic;
	 Moderately sticky; Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change 
	to - 
	A2	0.2 - 0.42 m	Pale brown (10YR6/3-Moist); Very pale brown (10YR8/3-Dry); Mottles, 0-2% , Distinct; Sandy 
	loam; Massive grade of structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-
	1mm) macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Slightly plastic; 
	Moderately sticky; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments;
	 Few (2 - 10 %), Unidentified, Fine (0 - 2 mm), Nodules, strong, segregations;Few (2 - 10 %), 
	Unidentified, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6.5 (Raupach); 
	Common, fine (1-2mm) roots; Clear change to - 
	B	0.42 - 0.7 m	Yellowish brown (10YR5/4-Moist); Mottles, 20-50% , Faint; Light medium clay; Moderate grade of
	 structure, 20-50 mm, Angular blocky; 100-200 mm, Lenticular; Smooth-ped fabric; Common (1-5
	 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Moderately plastic; Very sticky; 0-2%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; Very few (0 - 2 %), Unidentified, Fine (0 - 2 mm), Nodules, 
	strong, segregations;Very few (0 - 2 %), Unidentified, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 7.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Artificial drainage exposure.                                                                                                                                                               
	            
	Site Notes
	30M IN FENCE                          

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW218	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile