Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	276 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6083250 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	522600  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Ou	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Chromosol Thick Gravelly Loamy  	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	Non-calcic brown 
	Confidence level not specified	soil
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.15 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Weak grade of structure, 20-50 mm, Subangular
	 blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common 
	(1-5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Slightly plastic; Moderately 
	sticky; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, 
	segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 5 (Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	B2	0.15 - 0.55 m	Yellowish red (5YR4/8-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Moderately plastic; Very sticky; Very few 
	(0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %),
	 Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Diffuse change to - 
	B3	0.55 - 1.1 m	Strong brown (7.5YR4/6-Moist); Mottles, 2-10% , Distinct; Mottles, 2-10% , Faint; Light medium 
	clay; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Common (1-5 per 
	100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Moderately plastic; Very sticky; Very few (0 - 2 %), Ferromanganiferous, Fine (0
	 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules, strong, segregations;Field pH 7 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Bedrock exposed 20m away, near crest.                                                                                                                                            
	                       
	Site Notes
	END OF SEALED ROAD, W SIDE            

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW229	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile