Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW279	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	192 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6102875 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	504300  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Stable, Present (stbank) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Red Chromosol Thick Moderately gravelly Peaty  	Principal Profile Form:	Dr2.22
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.4 m	Brown (7.5YR4/3-Moist); ; Fine sandy loam; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common 
	(1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Non-plastic; Slightly 
	sticky; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Diffuse, Smooth change to - 
	A2	0.4 - 0.65 m	Brown (7.5YR5/4-Moist); Reddish yellow (7.5YR6/6-Dry); ; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; Non-plastic; 
	Slightly sticky; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B2	0.65 - 0.8 m	Yellowish red (5YR4/6-Moist); ; Clay loam, sandy; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) 
	macropores, Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; 
	Moderately plastic; Moderately sticky; Field pH 7 (Raupach); Few, fine (1-2mm) roots; Clear, 
	Smooth change to - 
	B3	0.8 - 1.05 m	Brown (7.5YR5/4-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-
	2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; Field pH 6.5 
	(Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	River bank exposure.River bottom 6m below alluvial plain                                                                                                                 
	                               
	Site Notes
	150M IN FENCE                         

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW279	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW279	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile