Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	230 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6108575 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	513775  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgc	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	12 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.12
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subrounded, Quartz; No surface coarse fragments
	Profile Morphology
	A	0 - 0.15 m	Dark brown (10YR3/3-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy fabric;
	 Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Moderately moist; Firm consistence; Slightly plastic; Normal plasticity; Slightly 
	sticky; 0-2%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 5 
	(Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	B	0.15 - 0.35 m	Yellowish brown (10YR5/6-Moist); Mottles, 10-20% , Prominent; Medium clay; Weak grade of 
	structure, 5-10 mm, Platy; 100-200 mm, Lenticular; Smooth-ped fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately 
	moist; Very firm consistence; Very plastic; Normal plasticity; Very sticky; 0-2%, fine gravelly, 2-
	6mm, subrounded, dispersed, Quartz, coarse fragments; Field pH 7 (Raupach); Common, fine 
	(1-2mm) roots; Diffuse, Smooth change to - 
	C	0.35 - 0.7 m	Dark red (2.5YR3/6-Moist); Mottles, 10-20% , Prominent; Medium heavy clay; Weak grade of 
	structure, 5-10 mm, Platy; 100-200 mm, Lenticular; Smooth-ped fabric; Moderately moist; Very 
	firm consistence; Very plastic; Normal plasticity; Very sticky; 0-2%, fine gravelly, 2-6mm, 
	subrounded, dispersed, Quartz, coarse fragments; Field pH 6.5 (Raupach); Few, fine (1-2mm) 
	roots; 
	Morphological Notes
	Observation Notes
	Further West - red earth                Further East - siliceous sand on grey   clay                                                                                  
	                                  
	Site Notes
	OPPOSITE PAYNES ROAD                  

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW29	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile