Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW299	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	259 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6096925 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	521475  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgr	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	7 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Brown Chromosol Thick Non-gravelly Loamy Clayey	Principal Profile Form:	Dy2.42
	 Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.2 m	Dark brown (7.5YR3/3-Moist); ; Loam; Weak grade of structure, 5-10 mm, Subangular blocky; 
	Earthy fabric; Many (>5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Dry; Firm consistence; Slightly plastic; Slightly sticky; 
	Field pH 5.5 (Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	A2	0.2 - 0.35 m	Brown (7.5YR5/3-Moist); Pink (7.5YR7/4-Dry); ; Clay loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Few (<1 per 100mm2) 
	Fine (1-2mm) macropores, Dry; Weak consistence; Slightly plastic; Moderately sticky; 10-20%, 
	fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6.5 (Raupach); 
	Few, fine (1-2mm) roots; Abrupt, Smooth change to - 
	B	0.35 - 0.5 m	Yellowish brown (10YR5/4-Moist); Mottles, 2-10% , Faint; Medium clay; Moderate grade of 
	structure, 20-50 mm, Subangular blocky; Rough-ped fabric; Few (<1 per 100mm2) Very fine 
	(0.075-1mm) macropores, Dry; Strong consistence; Moderately plastic; Very sticky; 2-10%, fine 
	gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Fine (0 - 2 mm), Nodules, strong, segregations;Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6.5 (Raupach); 
	Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW299	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW299	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile