Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	292 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6088450 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	513075  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ou	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	No Data
	Slope:	5 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy2.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (7.5YR3/3-Moist); ; Medium sandy clay loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Moist; Slightly plastic; Moderately sticky; Field pH 5.5 
	(Raupach); Common, fine (1-2mm) roots; Gradual change to - 
	A2	0.15 - 0.6 m	Brown (7.5YR5/4-Moist); Pinkish grey (7.5YR7/3-Dry); ; Clay loam, sandy; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Moderately plastic; 
	Very sticky; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, 
	segregations;Field pH 6 (Raupach); Common, fine (1-2mm) roots; Gradual change to - 
	B	0.6 - 0.8 m	Light yellowish brown (10YR6/4-Moist); Mottles, 2-10% , Faint; Medium heavy clay; Moderate 
	grade of structure, 5-10 mm, Polyhedral; Smooth-ped fabric; Moderately moist; Very plastic; Very
	 sticky; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 mm), Soft segregations, weak, 
	segregations;Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Soft segregations, 
	weak, segregations;Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Pit to 40cm                             Auger to 80cm                                                                                                                                     
	              
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW34	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile