Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	292 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6091350 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	509275  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ou	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	10 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Active, Moderate (sheet) Active, Moderate (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.12
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, angular, ; No surface coarse fragments
	Profile Morphology
	A	0 - 0.3 m	Very dark brown (7.5YR2/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Few (<1
	 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Moderately plastic; Moderately sticky; 
	20-50%, medium gravelly, 6-20mm, angular, dispersed, coarse fragments; Field pH 5.5 
	(Raupach); Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B	0.3 - 0.95 m	Dark red (2.5YR3/6-Moist); Mottles, 2-10% , Distinct; Medium heavy clay; Moderate grade of 
	structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Moist; Very plastic; Very sticky; 2-10%, 
	medium gravelly, 6-20mm, angular, dispersed, coarse fragments; Few cutans, <10% of ped 
	faces or walls coated, faint; Field pH 6.5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A	A recent colluvial layer.               Metasedimentary rock gravels.                                         
	                                                                                          
	B	Much older than layer 1.                Metasedimentary rock gravels.                                        
	                                                                                           
	Observation Notes
	Site Notes
	40M DOWN SLOPE FROM GATE              

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW40	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile