Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	309 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6085350 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	535800  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Silt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	1 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Active, Present (stbank) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.84
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.22 m	Very dark brown (10YR2/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Polyhedral; 
	Earthy fabric; Fine, (0 - 5) mm crack; Common (1-5 per 100mm2) Fine (1-2mm) macropores, 
	Moist; Slightly plastic; Slightly sticky; Field pH 6 (Raupach); Many, fine (1-2mm) roots; Gradual 
	change to - 
	A2	0.22 - 0.44 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Fine, (0 - 5) mm 
	crack; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moist; Slightly plastic; Slightly 
	sticky; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Gradual change to - 
	B2	0.44 - 0.75 m	Dark greyish brown (10YR4/2-Moist); Mottles, 2-10% , Distinct; Silty clay loam; Massive grade of 
	structure; Earthy fabric; Fine, (0 - 5) mm crack; Many (>5 per 100mm2) Fine (1-2mm) macropores,
	 Moist; Moderately plastic; Moderately sticky; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 
	mm), Soft segregations, weak, segregations;Field pH 6 (Raupach); Few, fine (1-2mm) roots; 
	Gradual change to - 
	B3	0.75 - 1.6 m	Yellowish brown (10YR5/4-Moist); Mottles, 10-20% , Distinct; Clay loam, sandy; Moderate grade 
	of structure, 50-100 mm, Columnar; Smooth-ped fabric; Fine, (0 - 5) mm crack; Moderately moist;
	 Moderately plastic; Moderately sticky; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 
	mm), Soft segregations, weak, segregations;Field pH 6 (Raupach); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW53	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile