Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	250 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6090800 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	538075  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Channel bench	Slope Category:	No Data
	Slope:	2 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Partial, Present (stbank) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.21
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.3 m	Dark reddish brown (5YR3/3-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 100mm2) Coarse (>5mm) 
	macropores, Moist; Moderately plastic; Moderately sticky; Field pH 6 (Raupach); Many, very fine 
	(0-1mm) roots; Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	B	0.3 - 1 m	Strong brown (7.5YR5/6-Moist); ; Silty clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Few (<1 per 100mm2) Coarse (>5mm) 
	macropores, Moist; Moderately plastic; Moderately sticky; Field pH 6 (Raupach); Common, very 
	fine (0-1mm) roots; Common, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes
	30M S OF BRIDGE                       

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.3	5.1B	0.09A	4.5J	1.4	1	0.4	0L	6.9I	5.80
	0.3 - 1	5.7B	0.06A	3.3J	0.9	0.4	0.3	0L	4.2I	7.14
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.3	1.61A	5D	9F	61	17	13
	0.3 - 1	0.17A	1D	4F	56	22	18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.3	0.48B	0.11B
	0.3 - 1	0.34B	0.09B

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F2	Exchangeable aluminium by 0.01m (AgTU)+
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	3A1	EC of 1:5 soil/water extract
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9E	Available P (mg/kg) - Bray P
	9J2	Phosphate sorption curve - automated colour
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_CS	Coarse Sand (%) - Hydrometer Method
	P10_HYD_FS	Fine Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3B_GV_01	0.1 BAR Moisture g/g - Gravimetric  using suction plate
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate