Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	255 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6090750 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	535375  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Cza	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.12
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.2 m	Brown (7.5YR4/3-Moist); ; Clay loam; Weak grade of structure, 2-5 mm, Polyhedral; Earthy fabric;
	 Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) 
	Fine (1-2mm) macropores, Moist; Moderately plastic; Moderately sticky; Field pH 5 (Raupach); 
	Many, fine (1-2mm) roots; Clear, Smooth change to - 
	B2	0.2 - 0.55 m	Brown (7.5YR5/4-Moist); Mottles, 2-10% , Distinct; Medium heavy clay; Moderate grade of 
	structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Moist; Very plastic; Very sticky; 2-
	10%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Very few (0 - 2 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 6 (Raupach); 
	Common, fine (1-2mm) roots; Few, coarse (>5mm) roots; Gradual, Smooth change to - 
	B3	0.55 - 0.75 m	Brown (10YR5/3-Moist); Mottles, 10-20% , Faint; Coarse sandy light medium clay; Moderate 
	grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Moist; Moderately plastic; Moderately
	 sticky; 10-20%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; Very 
	few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules, strong, segregations;Field pH 
	6.5 (Raupach); Few, fine (1-2mm) roots; Few, coarse (>5mm) roots; 
	Morphological Notes
	Observation Notes
	Pit to 30cm, auger to 75cm.             Some disturbance of topsoil?                                                                                                   
	                                 
	Site Notes
	400M E OF DAM                         

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW58	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile