Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	30/08/87	Elevation:	440 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5878760 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	733790  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	DGWA	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	28 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Stable, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.34
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, subangular, Siltstone; No surface coarse fragments
	Profile Morphology
	O1	0 - 0.04 m	Organic Layer; ; Medium sandy clay loam; Moderately moist; Clear, Smooth change to - 
	A1	0.04 - 0.13 m	Brown (10YR4/3-Moist); ; Medium sandy clay loam; Weak grade of structure, 2-5 mm, Granular; 
	Earthy fabric; Moderately moist; Very weak consistence; 2-10%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; 2-10%, coarse gravelly, 20-60mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 6 (Raupach); Many, very fine (0-1mm)
	 roots; Many, medium (2-5mm) roots; Gradual, Wavy change to - 
	A2c	0.13 - 0.3 m	Light yellowish brown (10YR6/4-Moist); ; Medium sandy clay loam; Moderate grade of structure, 
	10-20 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, subangular, dispersed, Siltstone, coarse fragments; 2-10%, coarse gravelly, 
	20-60mm, subangular, dispersed, Siltstone, coarse fragments; 2-10%, fine gravelly, 2-6mm, 
	angular, dispersed, Siltstone, coarse fragments; Field pH 6 (Raupach); Common, fine (1-2mm) 
	roots; Common, medium (2-5mm) roots; Clear, Irregular change to - 
	B1	0.3 - 0.54 m	Brownish yellow (10YR6/6-Moist); ; Clay loam; Weak grade of structure, 20-50 mm, Polyhedral; 
	Earthy fabric; Moist; Firm consistence; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, 
	Siltstone, coarse fragments; 10-20%, cobbly, 60-200mm, subangular, dispersed, Siltstone, 
	coarse fragments; 10-20%, fine gravelly, 2-6mm, angular, dispersed, Siltstone, coarse 
	fragments; Field pH 6 (Raupach); Common, fine (1-2mm) roots; Common, medium (2-5mm) 
	roots; Gradual, Irregular change to - 
	B21	0.54 - 0.79 m	Yellowish brown (10YR5/8-Moist); ; Clay loam; Weak grade of structure, 5-10 mm, Polyhedral; 
	Earthy fabric; Moist; Firm consistence; 20-50%, cobbly, 60-200mm, angular, dispersed, 
	Siltstone, coarse fragments; Field pH 6 (Raupach); Common, coarse (>5mm) roots; 
	B22	0.79 - 1.24 m	Brownish yellow (10YR6/8-Moist); ; Massive grade of structure; Earthy fabric; Firm consistence; 
	20-50%, cobbly, 60-200mm, angular, dispersed, Siltstone, coarse fragments; Field pH 5 
	(Raupach); Common, coarse (>5mm) roots; 
	Morphological Notes
	B1	Quartz grains diminish markedly in B2   horizon.                                                                  
	                                                                                      
	Observation Notes
	Pendent of Devonian (Merimbula) PM down-slope of hillcrest. Large boulders      throughout profile.                     Sedimentary 
	rock outcrop.                                                       

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	DP42 - near crest of major hill       

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.04 - 0.12	3.83I	1.65F	1.33	0.37	0.15	0.51G
	4.82H
	0.13 - 0.3	3.65I	0.47F	0.51	0.2	0.1	0.7G
	4.88H
	0.34 - 0.42	3.99I	0.56F	0.6	0.24	0.07	0.4G
	5.18H
	0.79 - 1.24	3.63I	0.96F	3.57	0.38	0.18	4.55G
	4.94H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.04 - 0.12	5.55A	41F	<0.01E	20
	0.13 - 0.3	0.94A	26F	<0.01E	28.4
	0.34 - 0.42	1.26A	32F	<0.01E	34.5
	0.79 - 1.24	0.45A	95F	<0.01E	20.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.04 - 0.12
	0.13 - 0.3
	0.34 - 0.42
	0.79 - 1.24

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA33	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	2A1	Air-dry moisture content
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)