Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	07/09/87	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5877130 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	733540  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Dgwa	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Open depression (vale)	Relief:	0 metres
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	15 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc2.23
	ASC Confidence:	Great Soil Group:	Humic gley
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	10-20%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.07 m	Very dark grey (10YR3/1-Moist); ; Coarse sandy clay loam; Weak grade of structure, 5-10 mm, 
	Polyhedral; Earthy fabric; Moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 5 (Raupach); Many, fine (1-2mm) roots; Many, 
	medium (2-5mm) roots; Many, coarse (>5mm) roots; Clear, Smooth change to - 
	A12	0.07 - 0.22 m	Weak red (2.5YR5/2-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moist; Weak consistence; 10-20%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse 
	fragments; Field pH 5.5 (Raupach); Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Gradual, Smooth change to - 
	A21c	0.22 - 0.4 m	Pale red (2.5YR6/2-Moist); ; Coarse sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 6 (Raupach); Few, fine (1-2mm) roots; Few, 
	medium (2-5mm) roots; Gradual, Wavy change to - 
	A22	0.4 - 0.6 m	Pale red (2.5YR7/2-Moist); , 10-20% , Distinct; Coarse sandy loam; Massive grade of structure; 
	Sandy (grains prominent) fabric; Wet; Weak consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, fine (1-2mm) 
	roots; Clear, Irregular change to - 
	B2	0.6 - 0.95 m	Pale red (2.5YR7/2-Moist); , 20-50% , Distinct; Clayey coarse sand; Massive grade of structure; 
	Earthy fabric; Moist; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, undisturbed, 
	Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 
	(Raupach); Few, medium (2-5mm) roots; 
	Morphological Notes
	Observation Notes
	Heath-Meleu. Scrub drainage flat. Collu-vial sand over in situ B horizon. Perch-ed water-table over B2 horizon. Rust    coating 
	adjacent to root in A horizons. A2 horizons dispersive.                 
	Site Notes
	DP64 - suspended drainage line        

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	3.63I	0.69F	0.38	0.14	0.09	0.58G
	4.64H
	0.3 - 0.38	3.84I	0.07F	0.37	0.08	0.04	0.28G
	5.07H
	0.4 - 0.6	3.9I	0.05F	0.46	0.1	0.03	0.29G
	5.17H
	0.6 - 0.95	3.83I	0.03F	0.82	0.08	0.05	0.47G
	5.03H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	3.47A	30F	<0.01E	8
	0.3 - 0.38	0.39A	9F	<0.01E	17.1
	0.4 - 0.6	0.45A	10F	<0.01E	28.8
	0.6 - 0.95	0.24A	7F	<0.01E	22.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.3 - 0.38
	0.4 - 0.6
	0.6 - 0.95

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)