Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	08/09/87	Elevation:	210 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5876130 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	734810  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	0 metres
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	9 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments; 20-50%, , subangular, Quartz; 20-50%, , rounded, Quartz
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; Medium sandy clay loam; Moist; Clear, Wavy change to - 
	A1	0.02 - 0.28 m	Very dark grey (10YR3/1-Moist); ; Sandy loam; Moderate grade of structure, 5-10 mm, Polyhedral;
	 Rough-ped fabric; Moist; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; 20-50%, medium gravelly, 6-20mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 4 (Raupach); Many, fine (1-2mm) roots; Many, 
	medium (2-5mm) roots; Many, coarse (>5mm) roots; Abrupt, Wavy change to - 
	A2c	0.28 - 0.37 m	Light grey (10YR7/2-Moist); ; Medium sandy clay loam; Weak grade of structure, 10-20 mm, 
	Polyhedral; Earthy fabric; Moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few,
	 coarse (>5mm) roots; Gradual, Wavy change to - 
	B1h	0.37 - 0.48 m	Brownish yellow (10YR6/6-Moist); , 10-20% , Distinct; , 10-20% , Faint; Medium sandy clay; 
	Moderate grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Moist; Firm consistence; 
	20-50%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Few cutans, 
	<10% of ped faces or walls coated, distinct; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 
	mm), Soft segregations, weak, segregations;Common (10 - 20 %), Ferruginous, Coarse (6 - 20 
	mm), Nodules, weak, segregations;, Organic (humified), , ; Field pH 5.5 (Raupach); Common, 
	fine (1-2mm) roots; Common, medium (2-5mm) roots; Common, coarse (>5mm) roots; Clear, 
	Smooth change to - 
	B2	0.48 - 0.82 m	Yellowish brown (10YR5/8-Moist); , 10-20% , Distinct; Moderate grade of structure, 5-10 mm, 
	Polyhedral; Smooth-ped fabric; Firm consistence; 20-50%, fine gravelly, 2-6mm, subangular, 
	dispersed, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; 
	Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Nodules, weak, segregations;Field pH 5 
	(Raupach); Common, fine (1-2mm) roots; Common, medium (2-5mm) roots; 
	Morphological Notes
	O1	Dominant ped size also 10-20mm.         Casts common.                           Varigated 
	faunal mixing.                                                                                                
	A2c	dominant ped size also 10-20mm.                                                                                       
	                                                                                  
	B1h	Dominant ped size also 10-20mm.                                                                                       

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Slight development of podzol horizon.                                                                                                                                                
	                   
	Site Notes
	DP11 - open drainage depression       
	Observation Notes

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.1	3.12I	0.77F	0.44	0.15	0.04	0.74G
	4.04H
	0.28 - 0.37	3.69I	0.17F	0.22	0.13	0.03	0.71G
	4.56H
	0.32 - 0.4	3.9I	0.16F	0.28	0.17	0.03	0.99G
	4.73H
	0.37 - 0.48	3.98I	0.13F	0.29	0.21	0.04	1.12G
	4.8H
	0.48 - 0.82	3.89I	0.31F	1.81	0.55	0.16	2.07G
	4.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.1	5.66A	32F	<0.01E	19.9
	0.28 - 0.37	0.77A	20F	<0.01E	30
	0.32 - 0.4	0.94A	15F	<0.01E	32
	0.37 - 0.48	0.97A	16F	<0.01E	34.1
	0.48 - 0.82	0.95A	28F	<0.01E	16.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.1
	0.28 - 0.37
	0.32 - 0.4
	0.37 - 0.48
	0.48 - 0.82

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA52	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)