Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA57	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	09/09/87	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8823   1:25000	Rainfall:	No Data
	Northing/Long.:	5878270 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	734490  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	0 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	35 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Uc4.24
	ASC Confidence:	Great Soil Group:	Lithosol
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subangular, Quartz; No surface coarse fragments
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; Sandy loam; Moist; Clear, Smooth change to - 
	A1	0.03 - 0.15 m	Very dark grey (10YR3/1-Moist); ; Medium sandy clay loam; Weak grade of structure, 10-20 mm, 
	Polyhedral; Earthy fabric; Moist; Very weak consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 4 (Raupach); Common, very fine (0-
	1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-5mm) roots; Gradual, Wavy 
	change to - 
	A2	0.15 - 0.23 m	Dark greyish brown (10YR4/2-Moist); ; Medium sandy clay loam; Weak grade of structure, 5-10 
	mm, Polyhedral; Earthy fabric; Moist; Firm consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular, dispersed, Quartz, coarse fragments; 20-50%, medium gravelly, 6-20mm, 
	subangular, dispersed, Quartz, coarse fragments; Field pH 5 (Raupach); Common, medium (2-
	5mm) roots; Common, coarse (>5mm) roots; Abrupt, Wavy change to - 
	B2	0.23 - 0.53 m	Yellowish brown (10YR5/4-Moist); ; Weak grade of structure, 5-10 mm, Polyhedral; Earthy fabric;
	 Weak consistence; 20-50%, fine gravelly, 2-6mm, subrounded, dispersed, coarse fragments; 
	20-50%, medium gravelly, 6-20mm, subrounded, dispersed, coarse fragments; 20-50%, fine 
	gravelly, 2-6mm, subangular, dispersed, coarse fragments; Field pH 5 (Raupach); Common, 
	medium (2-5mm) roots; Common, coarse (>5mm) roots; 
	Morphological Notes
	A1	Dominant ped size also 10-20mm.                                                                                       
	                                                                                  
	A2	Dominant ped size also 10-20mm.                                                                                       
	                                                                                  
	Observation Notes
	Shallow profile resting on rock.                                                                                                                                                          
	              
	Site Notes
	DP94 - steep lower slope above dry crk

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA57	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.11	3.03I	0.79F	1.25	0.37	0.15	1.33G
	3.86H
	0.15 - 0.23	3.71I	0.33F	0.37	0.11	0.06	0.94G
	4.62H
	0.33 - 0.41	4.11I	0.05F	0.21	0.12	0.06	1.22G
	4.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.11	9.39A	51F	<0.01E	22.1
	0.15 - 0.23	1.68A	28F	<0.01E	24.4
	0.33 - 0.41	1.5A	35F	<0.01E	31
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.11
	0.15 - 0.23
	0.33 - 0.41

	Project Name:	EDEN BURNING STUDY AREA                 
	Project Code:	1000638	Site ID:	EDB_SA57	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15D1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for 
	soluble salts; manual leach
	15D1_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15D1_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	manual leach
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By
	 AAS
	4A_C_1	pH of soil - pH of 1:1 soil/water suspension
	4C_C_1	pH of 1:1 soil/1M potassium chloride suspension
	6A1	Organic carbon - Walkley and Black
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)