Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	A32	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Gunn, RH	Locality:	Profile A32 located 11.2 km north of Wallumbilla.
	Date Desc.:	01/01/74	Elevation:	No Data
	Map Ref.:	Sheet No. : SG55-12   1:250000	Rainfall:	600
	Northing/Long.:	149.2186194	Runoff:	No Data
	Easting/Lat.:	-26.44579816	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Red Sodosol     	Principal Profile Form:	Dr2.23
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Mid Strata - Shrub, , Sparse. *Species includes - Eremophila mitchellii, Geijera parviflora
	Tall Strata - Tree, , Mid-dense. *Species includes - Casuarina cristata
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy clay loam; Massive grade of structure; Weak 
	consistence; 
	A2	0.13 - 0.2 m	Reddish brown (5YR4/3-Moist); Brown (7.5YR4/4-Dry); ; Fine sandy loam; Massive grade of 
	structure; Firm consistence; 
	B21	0.2 - 0.66 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; , Angular blocky; Strong consistence; 
	B22	0.66 - 1.07 m	Reddish brown (5YR4/4-Moist); ; Medium heavy clay; , Angular blocky; Strong consistence; Few 
	(2 - 10 %), Calcareous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	A32	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6A	4A	2.4	0.96
	0.13 - 0.2	7.3A
	0.2 - 0.66	7.5A	0.53A	2.9A	9.6	0.45
	0.66 - 1.07	9.2A	0.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	1.3A
	0.13 - 0.2
	0.2 - 0.66
	0.66 - 1.07
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.2
	0.2 - 0.66
	0.66 - 1.07

	Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	A32	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	9G1	Acid-extractable phosphorus - manual colour