Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	H27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Gunn, RH	Locality:	Profile H27 located 3.2 km south of "Somerset HS.
	Date Desc.:	01/01/74	Elevation:	No Data
	Map Ref.:	Sheet No. : SH55-3   1:250000	Rainfall:	430
	Northing/Long.:	148.2965103	Runoff:	No Data
	Easting/Lat.:	-28.93223786	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - Astrebla species
	Tall Strata - Tree, , Very sparse. *Species includes - Eucalyptus microtheca, Acacia pendula
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.01 m	Dark grey (10YR4/1-Moist); ; Medium clay; Weak grade of structure, Platy; , Granular; Very weak 
	consistence; 
	B1	0.01 - 0.15 m	Dark grey (10YR4/1-Moist); ; Medium clay; , Subangular blocky; Strong consistence; 
	B21	0.15 - 0.46 m	Dark grey (10YR4/1-Moist); ; Medium heavy clay; , Subangular blocky; Strong consistence; 
	B22	0.46 - 0.9 m	Grey (10YR5/1-Moist); ; Medium heavy clay; , Subangular blocky; Strong consistence; Few (2 - 
	10 %), Calcareous, , Soft segregations; 
	B23	0.9 - 1.5 m	Grey (10YR5/1-Moist); ; Heavy clay; Massive grade of structure; Firm consistence; Few (2 - 10 
	%), Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	H27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	8.3A	31.8A	7.8	1.58
	0.01 - 0.15	8.3A	31.8A	7.8	1.58
	0.15 - 0.46	8.7A	0.26A
	0.46 - 0.9	8.5A	26.2A	11.5	0.98
	0.9 - 1.5	8.3A	1.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	0.7A
	0.01 - 0.15	0.7A
	0.15 - 0.46
	0.46 - 0.9
	0.9 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.15
	0.15 - 0.46
	0.46 - 0.9
	0.9 - 1.5

	Project Name:	Balonne-Maranoa Soil Survey and Soil Moisture Profiles
	Project Code:	B-M	Site ID:	H27	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	9G1	Acid-extractable phosphorus - manual colour