Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	05/04/95	Elevation:	1193 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6043735 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	611736  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	SGGH	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	17 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Medium Non-gravelly Clayey 	Principal Profile Form:	Gn2.11
	Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	0-2%, cobbly, 60-200mm, subangular tabular, 
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	A1	0.03 - 0.15 m	Dark reddish brown (5YR3/2-Moist); Biological mixing, 10-20% , Faint; Biological mixing, 10-
	20% , Faint; Light clay; Strong grade of structure, 2-5 mm, Polyhedral; 100-200 mm, Prismatic; 
	Rough-ped fabric; Moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, subangular 
	tabular, dispersed, coarse fragments; Field pH 6 (pH meter); Common, very fine (0-1mm) roots; 
	Common, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; Clear, 
	Smooth change to - 
	B1	0.15 - 0.28 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 2-10% , Distinct; Fine sandy light clay; 
	Moderate grade of structure, 5-10 mm, Polyhedral; 50-100 mm, Columnar; Smooth-ped fabric; 
	Moderately moist; Weak consistence; 0-2%, coarse gravelly, 20-60mm, subangular tabular, 
	dispersed, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 
	5.5 (pH meter); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Common, medium (2-
	5mm) roots; Few, coarse (>5mm) roots; Clear, Irregular change to - 
	B21	0.28 - 0.53 m	Yellowish red (5YR4/6-Moist); Biological mixing, 0-2% , Distinct; Clay loam, sandy; Weak grade 
	of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Firm 
	consistence; 0-2%, coarse gravelly, 20-60mm, subangular tabular, dispersed, coarse 
	fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (pH meter); Few, 
	very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Diffuse, Smooth change to - 
	B22	0.53 - 0.78 m	Yellowish red (5YR4/6-Moist); Biological mixing, 0-2% , Faint; Clay loam, sandy; Massive grade 
	of structure; Earthy fabric; Moderately moist; Weak consistence; 0-2%, coarse gravelly, 20-
	60mm, subangular tabular, dispersed, coarse fragments; 0-2%, medium gravelly, 6-20mm, 
	angular tabular, dispersed, Coal, coarse fragments; Field pH 5 (pH meter); Few, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Gradual, Irregular change to - 
	B23	0.78 - 1.28 m	Yellowish red (5YR4/6-Moist); Substrate influence, 2-10% , Faint; Fine sandy clay loam; 
	Massive grade of structure; Earthy fabric; Moderately moist; Weak consistence; 0-2%, coarse 
	gravelly, 20-60mm, subangular tabular, dispersed, coarse fragments; 0-2%, medium gravelly, 6-
	20mm, angular tabular, dispersed, Coal, coarse fragments; 2-10%, coarse gravelly, 20-60mm, 
	subrounded tabular, dispersed, coarse fragments; Field pH 5 (pH meter); Few, very fine (0-1mm) 
	roots; Diffuse change to - 

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B3	1.28 - 1.98 m	Strong brown (7.5YR4/6-Moist); ; Fine sandy clay loam; Earthy fabric; 2-10%, coarse gravelly, 20-
	60mm, subrounded tabular, dispersed, coarse fragments; Field pH 5 (pH meter); 
	Morphological Notes
	B23	Increase in course fragments of feldspar10 to 20%, 6 - 20 mm. Mafic substrate 
	increases in abundance in this layer and below.
	Observation Notes
	PGP centre peg 6 m south west. Wet ash site.
	Site Notes
	PGP18, BAGO S.F., COMPT 94

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.11	4.39C	2.27H	0.65	0.66	0.02	3.35J	6.94E
	5.22A	0K
	0.18 - 0.28	4.39C	1H	0.53	0.45	0.01	1.4J	3.4E
	5.31A	0K
	0.33 - 0.41	4.35C	0.98H	0.65	0.52	0.02	1.39J	3.56E
	5.41A	0K
	0.53 - 0.63	4.07C	0.14H	0.17	0.47	0	2.48J	3.26E
	5.14A	0K
	0.83 - 1.03	4.08C	0.05H	0.2	0.26	0	2.16J	2.67E
	5.16A	0K
	1.53 - 1.83	4.13C	0.04H	0.18	0.25	0.03	1.69J	2.2E
	5.17A	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.11	4.04B	488.5B	0.21A	1.08	16.99
	0.18 - 0.28	1.42B	347.9B	0.08A	1.39	7.79
	0.33 - 0.41	0.84B	313.5B	0.05A	1.25	6.66
	0.53 - 0.63	0.35B	278.7B	0.02A	1.32	4.01
	0.83 - 1.03	0.1B	262.4B	0.01A	1.64	10.84
	1.53 - 1.83	0.09B	308.3B	0.01A	10.74
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.11
	0.18 - 0.28
	0.33 - 0.41
	0.53 - 0.63
	0.83 - 1.03
	1.53 - 1.83

	Project Name:	BAGO-MARAGLE ESM
	Project Code:	BGM_ESM	Site ID:	1025	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3