Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0034	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	23/11/95	Elevation:	1267 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6034104 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	617384  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Os	Substrate Material:	Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Medium Slightly gravelly 	Principal Profile Form:	Uf6.71
	Clayey Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, subangular tabular, Sandstone
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	Ap	0.03 - 0.18 m	Dark reddish brown (5YR3/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 2-10%, coarse gravelly, 20-60mm, subrounded tabular, Sandstone, coarse 
	fragments; Field pH 5 (Raupach); Common, very fine (0-1mm) roots; Many, fine (1-2mm) roots; 
	Common, medium (2-5mm) roots; Few, coarse (>5mm) roots; Sharp, Smooth change to - 
	A1b	0.18 - 0.31 m	Dark reddish brown (5YR3/2-Moist); ; Clay loam; Moderate grade of structure, 5-10 mm, Angular 
	blocky; 2-5 mm, Polyhedral; Rough-ped fabric; Moist; Weak consistence; 0-2%, medium 
	gravelly, 6-20mm, angular, Quartz, coarse fragments; 2-10%, coarse gravelly, 20-60mm, 
	subrounded tabular, Sandstone, coarse fragments; Field pH 5 (Raupach); Common, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Common, medium (2-5mm) roots; Few, coarse (>5mm) 
	roots; Clear, Smooth change to - 
	B1b	0.31 - 0.48 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 5YR32, 20-50% , Faint; Light clay; 
	Moderate grade of structure, 5-10 mm, Polyhedral; 10-20 mm, Subangular blocky; Rough-ped 
	fabric; Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, subrounded tabular, 
	Sandstone, coarse fragments; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine 
	(1-2mm) roots; Common, medium (2-5mm) roots; Gradual, Wavy change to - 
	B2b	0.48 - 0.69 m	Dark red (2.5YR3/6-Moist); Biological mixing, 5YR32, 0-2% , Faint; Light clay; Massive grade of 
	structure; Earthy fabric; Moist; Weak consistence; 10-20%, medium gravelly, 6-20mm, 
	subrounded tabular, Sandstone, coarse fragments; Field pH 5 (Raupach); Few, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Gradual, Irregular change to - 
	BCb	0.69 - 0.88 m	Red (2.5YR4/6-Moist); ; Fine sandy clay; Massive grade of structure; Earthy fabric; Moist; Weak 
	consistence; 20-50%, coarse gravelly, 20-60mm, subangular tabular, Sandstone, coarse 
	fragments; Field pH 4.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Clear, 
	Irregular change to - 
	Morphological Notes
	Ap	Soil material of B horizon origin and has been transported over existing soil. No obvious 
	surface active erosion. Cause could be original logging event.
	A1b	Buried A horizon.                                                                                                                  
	                                                                     
	Observation Notes

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0034	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Area was logged 30-40 years ago. Recent regrowth indicates a second logging episode.
	Site Notes
	COMP 9H,2261-1,348D,50M FROM LOG. RD  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0034	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.03 - 0.18	3.97C	0.01H	0.29	0.54	0	4J	4.85E
	0K
	0.18 - 0.31	4.08C	0.03H	0.29	0.7	0	3.6J	4.63E
	0K
	0.31 - 0.48	4.08C	0H	0.23	0.58	0	2.87J	3.68E
	0K
	0.48 - 0.69	4.07C	0H	0.24	0.33	0	2.18J	2.75E
	0K
	0.69 - 0.88	4.02C	0H	0.24	0.26	0	2.29J	2.79E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.18	2.76B	299.5B	0.11A	0.95	20.27
	0.18 - 0.31	3.29B	350.6B	0.13A	1.15	28.22
	0.31 - 0.48	1.63B	279.8B	0.07A	1.30	26.82
	0.48 - 0.69	0.9B	244.9B	0.04A	1.11	32.43
	0.69 - 0.88	0.53B	248.5B	0.03A	1.24	26.4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.18
	0.18 - 0.31
	0.31 - 0.48
	0.48 - 0.69
	0.69 - 0.88

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0034	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3