Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0046	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	11/03/96	Elevation:	1224 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6038390 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	615878  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	13 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Thick Gravelly Clay-loamy 	Principal Profile Form:	Um6.
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	A11	0.03 - 0.13 m	Dark reddish brown (5YR3/3-Moist); Biological mixing, 5YR44, 20-50% , Distinct; Clay loam; 
	Moderate grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Dry; Firm consistence; 0-
	2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; 10-20%, stony, 200-
	600mm, subrounded, dispersed, Granodiorite, coarse fragments; Few cutans, <10% of ped 
	faces or walls coated, faint; Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Few, fine (1-
	2mm) roots; Clear, Smooth change to - 
	A12	0.13 - 0.38 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 5YR33, 20-50% , Distinct; Clay loam; 
	Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Dry; Weak consistence; 
	0-2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; 10-20%, stony, 200-
	600mm, subrounded, dispersed, Granodiorite, coarse fragments; Common cutans, 10-50% of 
	ped faces or walls coated, faint; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; Few, fine 
	(1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; Gradual, Smooth 
	change to - 
	B2	0.38 - 0.68 m	Red (2.5YR4/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Moderately moist; 
	Weak consistence; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 
	(Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; 
	Abrupt, Irregular change to - 
	C	0.68 - 1.43 m	Red (2.5YR4/6-Moist); ; Medium sandy clay loam; Massive grade of structure; Moderately moist; 
	Very weak consistence; Field pH 5 (Raupach); 
	Morphological Notes
	A11	Strongly hydrophobic.                                                                                                           
	                                                                        
	A12	Large dark worm casts from A1 horizon   - this could almost be an A3 or B1.                     
	                                                                                                        
	B2	Massive.                                                                                                                                
	                                                                
	C	Saprolite - strongly weathered granodiorite.
	Observation Notes
	A surprisingly shallow profile - strongly erosional site with v.dry north aspect. Large CFs. Local rise with outcropping rocks. 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0046	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	COMP 117H,11242-1,B 103,360M FR RD/CK 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0046	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.03 - 0.13	4C	1.61H	0.53	0.51	0.01	4.75J	7.41E
	0K
	0.13 - 0.38	4.11C	0.1H	0.57	0.62	0	3.41J	4.71E
	0K
	0.38 - 0.68	4.06C	0H	0.34	0.49	0	2.64J	3.47E
	0K
	0.68 - 1.43	4.12C	0H	0.21	0.35	0	1.23J	1.79E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.13	5.41B	339.6B	0.16A	0.95	36.73
	0.13 - 0.38	1.69B	384.3B	0.07A	1.14	25.4
	0.38 - 0.68	0.42B	276B	0.03A	1.24	18.93
	0.68 - 1.43	0.1B	152.4B	0.01A	1.71	20.84
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.13
	0.13 - 0.38
	0.38 - 0.68
	0.68 - 1.43

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0046	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3