Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0057	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	20/02/96	Elevation:	1181 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6027359 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	615098  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Dga	Substrate Material:	Adamellite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	19 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Loose
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Brown Dermosol Medium Slightly gravelly 	Principal Profile Form:	Gn4.8
	Loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	2-10%, cobbly, 60-200mm, subrounded tabular, Adamellite; 2-10%, cobbly, 60-200mm, subangular, Adamellite; 2-10%, 
	fine gravelly, 2-6mm, subangular tabular, Coal
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A1	0.02 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sandy loam; Single grain grade of structure; 
	Earthy fabric; Dry; Loose consistence; 2-10%, coarse gravelly, 20-60mm, subrounded, 
	Adamellite, coarse fragments; Field pH 5 (Raupach); Many, very fine (0-1mm) roots; Few, fine (1-
	2mm) roots; Few, medium (2-5mm) roots; Clear, Wavy change to - 
	A2	0.15 - 0.29 m	Brown (10YR4/3-Moist); Pale brown (10YR6/3-Dry); Biological mixing, 10YR32, 10-20% , 
	Distinct; Coarse sandy clay loam; Moderate grade of structure, 5-10 mm, Polyhedral; 2-5 mm, 
	Polyhedral; Rough-ped fabric; Moderately moist; Firm consistence; 20-50%, fine gravelly, 2-
	6mm, subangular, Quartz, coarse fragments; Field pH 5 (Raupach); Few, very fine (0-1mm) roots;
	 Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Gradual, Irregular change to - 
	B21t	0.29 - 0.56 m	Strong brown (7.5YR4/6-Moist); Biological mixing, 10YR32, 2-10% , Distinct; Coarse sandy clay;
	 Moderate grade of structure, 10-20 mm, Subangular blocky; 5-10 mm, Polyhedral; Rough-ped 
	fabric; Moderately moist; Firm consistence; 10-20%, medium gravelly, 6-20mm, subrounded, 
	Adamellite, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 4
	 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) 
	roots; Common, coarse (>5mm) roots; Diffuse, Irregular change to - 
	B22	0.56 - 1.27 m	Yellowish red (5YR5/8-Moist); ; Clay loam, sandy; Weak grade of structure, 5-10 mm, 
	Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; 10-20%, coarse gravelly, 
	20-60mm, subrounded, Adamellite, coarse fragments; Field pH 4.5 (Raupach); Few, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Diffuse change to - 
	B3	1.27 - 1.67 m	Strong brown (7.5YR5/8-Moist); ; Coarse sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Very weak consistence; 10-20%, medium gravelly, 6-20mm,
	 subangular, Adamellite, coarse fragments; 20-50%, fine gravelly, 2-6mm, subangular, Quartz, 
	coarse fragments; Field pH 4.5 (Raupach); Gradual change to - 
	Morphological Notes
	A1	Coarse textile indicates colluvial origin.
	B21t	Concentration of tree roots.                                                                                                  
	                                                                          
	Observation Notes

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0057	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Pit adjacent to large tors. Depth highly variable.                                                                                                                                
	                      
	Site Notes
	COMP 38H,3703-1,180DEG,1000M FROM ROAD

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0057	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.15	4.29C	9.83H	1.32	0.49	0	0.86J	13.58E
	1.08K
	0.15 - 0.29	4.13C	1.31H	0.37	0.39	0	2.2J	4.26E
	0K
	0.29 - 0.56	3.98C	0.72H	0.52	0.6	0.01	3.01J	4.85E
	0K
	0.56 - 1.27	3.9C	0H	0.12	0.82	0.04	3.58J	4.55E
	0K
	1.27 - 1.67	4.12C	0H	0.04	0.76	0.03	1.17J	2E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.15	7.59B	229.3B	0.25A	0.90	43.99
	0.15 - 0.29	2.13B	127.4B	0.07A	1.31	42.89
	0.29 - 0.56	1.14B	147B	0.05A	1.35	28.88
	0.56 - 1.27	0.49B	161B	0.03A	1.16	26.28
	1.27 - 1.67	0.11B	97.4B	0A	24.73
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.15
	0.15 - 0.29
	0.29 - 0.56
	0.56 - 1.27
	1.27 - 1.67

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0057	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3