Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0089	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	15/04/96	Elevation:	1122 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6041427 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	607632  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Tb	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	22 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Eutrophic Red Dermosol Medium Slightly 	Principal Profile Form:	Um6.33
	gravelly Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Chocolate soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.05 m	Organic Layer; ; 
	A1	0.05 - 0.16 m	Dark reddish brown (2.5YR3/3-Moist); Brown (7.5YR4/4-Dry); ; Silty clay loam; Moderate grade of 
	structure, <2 mm, Granular; 5-10 mm, Polyhedral; Rough-ped fabric; Moderately moist; Very 
	weak consistence; 2-10%, coarse gravelly, 20-60mm, subrounded tabular, Basalt, coarse 
	fragments; Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; 
	Few, medium (2-5mm) roots; Clear, Wavy change to - 
	B21	0.16 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Silty clay; Strong grade of structure, 2-5 mm, Polyhedral; 
	5-10 mm, Polyhedral; Rough-ped fabric; Moist; Very weak consistence; 2-10%, coarse gravelly, 
	20-60mm, subrounded tabular, Basalt, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Field pH 4.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm)
	 roots; Common, medium (2-5mm) roots; Few, coarse (>5mm) roots; Gradual, Smooth change to
	 - 
	B22	0.3 - 0.51 m	Dark reddish brown (2.5YR3/4-Moist); ; Silty clay; Strong grade of structure, 10-20 mm, 
	Subangular blocky; 5-10 mm, Polyhedral; Smooth-ped fabric; Moist; Very weak consistence; 
	Few cutans, <10% of ped faces or walls coated, distinct; Field pH 5 (Raupach); Many, very fine 
	(0-1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Gradual, Smooth change to - 
	B23	0.51 - 0.79 m	Dark reddish brown (2.5YR3/4-Moist); Biological mixing, 5YR32, 2-10% , Faint; Silty clay loam; 
	Strong grade of structure, 2-5 mm, Polyhedral; 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Weak consistence; Common cutans, 10-50% of ped faces or walls coated, 
	distinct; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; 
	Few, medium (2-5mm) roots; Gradual, Irregular change to - 
	B3	0.79 - 1.5 m	Dark reddish brown (2.5YR3/4-Moist); ; Silty clay loam; Strong grade of structure, 2-5 mm, 
	Polyhedral; 10-20 mm, Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 
	Common cutans, 10-50% of ped faces or walls coated, distinct; Field pH 5.5 (Raupach); 
	Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, 
	coarse (>5mm) roots; 
	Morphological Notes
	A1	Even after rain there are patches of dry hydrophobic soil below the litter. Little OM 
	accumulation so there could be active disturbance by lyrebirds and      wombats

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0089	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B21	Rest of profile is very moist.                                                                                                 
	                                                                         
	B3	Increase in large CFs.                                                                                                          
	                                                                        
	Observation Notes
	Hillslope with wombat holes and lyrebird activity. Site below mountain gum bole.                                                                           
	                                             
	Site Notes
	COMP 114H 42D 290M  FR/CR/RD 8576-1   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0089	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05
	0.05 - 0.16	4.52C	4.44H	2.22	1.29	0.21	2.52J	10.67E
	0K
	0.16 - 0.3	4.66C	4.46H	3.12	1.96	0.13	2.28J	11.95E
	0K
	0.3 - 0.51	4.56C	4.53H	3.57	1.7	0.13	1.68J	11.6E
	0K
	0.51 - 0.79	4.53C	4.58H	3.24	1.08	0.1	1.24J	10.23E
	0K
	0.79 - 1.5	4.49C	4.36H	3.5	0.84	0.15	1.39J	10.22E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.16	5.21B	2854.7B	0.16A	0.54	49.09
	0.16 - 0.3	2.61B	2774.4B	0.14A	0.91	27.01
	0.3 - 0.51	1.31B	1667.2B	0.1A	0.88	23.35
	0.51 - 0.79	0.84B	1465.3B	0.08A	0.89	26.71
	0.79 - 1.5	0.6B	1910.7B	0.06A	36.45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.16
	0.16 - 0.3
	0.3 - 0.51
	0.51 - 0.79
	0.79 - 1.5

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0089	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3