Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0095	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	16/04/96	Elevation:	1111 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6041744 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	605913  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Open depression (vale)	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	3 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Class Undetermined Redoxic Hydrosol Thick Non-	Principal Profile Form:	Um4.2
	gravelly Silty Clay-loamy Very deep
	ASC Confidence:	Great Soil Group:	Humic gley
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	O2	0.03 - 0.05 m	Organic Layer; ; 
	A11	0.05 - 0.21 m	Dark brown (7.5YR3/2-Moist); ; Silty clay loam; Weak grade of structure, 2-5 mm, Polyhedral; 
	Rough-ped fabric; Moist; Very weak consistence; Field pH 6 (Raupach); Many, very fine (0-1mm) 
	roots; Many, fine (1-2mm) roots; Common, medium (2-5mm) roots; Common, coarse (>5mm) 
	roots; Clear, Smooth change to - 
	A12	0.21 - 0.33 m	Very dark grey (7.5YR3/1-Moist); ; Silty clay loam; Moderate grade of structure, 2-5 mm, Granular;
	 5-10 mm, Polyhedral; Rough-ped fabric; Moist; Very weak consistence; Field pH 6 (Raupach); 
	Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-5mm) roots; 
	Few, coarse (>5mm) roots; Gradual, Smooth change to - 
	A13	0.33 - 0.51 m	Dark brown (7.5YR3/2-Moist); ; Clay loam; Moderate grade of structure, 10-20 mm, Angular 
	blocky; 2-5 mm, Polyhedral; Rough-ped fabric; Wet; Weak consistence; Field pH 6 (Raupach); 
	Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Few, medium (2-5mm) roots; 
	Few, coarse (>5mm) roots; Diffuse change to - 
	A21	0.51 - 0.95 m	Brown (7.5YR4/2-Moist); ; Medium sandy clay loam; Massive grade of structure; Earthy fabric; 
	Wet; Weak consistence; Field pH 6 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) 
	roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; Abrupt change to - 
	A22	0.95 - 1.55 m	Dark grey (10YR4/1-Moist); ; Clay loam; Moist; Field pH 6 (Raupach); Abrupt change to - 
	B2q	1.55 - 2 m	White (2.5Y8/1-Moist); Substrate influence, 7.5YR56, 10-20% , Prominent; Substrate influence, 
	2.5YR44, 2-10% , Prominent; Medium sandy clay loam; Moist; Field pH 7 (Raupach); 
	C	2 - 2.25 m	Reddish brown (2.5YR5/4-Moist); Substrate influence, 2.5YR44, 10-20% , Distinct; Substrate 
	influence, 10YR68, 10-20% , Distinct; Field pH 7 (Raupach); 
	Morphological Notes
	A11	A browner layer than that below and possibly recent deposition.
	A12	A darker A horizon                                                                                                                 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0095	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	A13	Less darker A.                                                                                                                       
	                                                                   
	A21	Paler and sand increases.                                                                                                   
	                                                                            
	A22	Sandy and waterlogged.                                                                                                       
	                                                                           
	B2q	Abrupt change to pale-gleyed soil. Sand decreases.                                                          
	                                                                                            
	C	Weathering Fe rich granodiorite.                                                                                          
	                                                                              
	Observation Notes
	Narrow drainage line upstream of flowing creek.
	Site Notes
	COMP113H 8078-1 166D 175M FROM RD/CK  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0095	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.05 - 0.21	4.57C	3.45H	2.65	0.34	0.06	1.27J	7.77E
	0K
	0.21 - 0.33	4.47C	3.25H	2.48	0.26	0.13	2.22J	8.34E
	0K
	0.33 - 0.51	4.4C	1.78H	1.96	0.16	0.16	1.91J	5.96E
	0K
	0.51 - 0.95	4.42C	1.53H	1.65	0.13	0.13	1.33J	4.79E
	0K
	0.95 - 1.55	4.45C	1.38H	1.37	0.09	0.24	0.98J	4.07E
	0K
	1.55 - 2	4.69C	1.43H	1.47	0.08	0.05	0.11J	3.25E
	0.11K
	2 - 2.25	5.01C	1.29H	1.22	0.08	0.16	0.05J	2.86E
	0.05K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.05 - 0.21	3.39B	1142.4B	0.21A	1.05	24.32
	0.21 - 0.33	3.18B	1328.3B	0.19A	0.93	41.79
	0.33 - 0.51	1.46B	1238.9B	0.09A	1.27	24.34
	0.51 - 0.95	1.23B	1141.4B	0.07A	21.49
	0.95 - 1.55	0.7B	762.7B	0.02A	21.7
	1.55 - 2	0.16B	121B	0.01A	20.1
	2 - 2.25	0.1B	544.5B	0A	26.12
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.05 - 0.21
	0.21 - 0.33
	0.33 - 0.51
	0.51 - 0.95
	0.95 - 1.55
	1.55 - 2
	2 - 2.25

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0095	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3