Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	17/04/96	Elevation:	1166 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6044709 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	605188  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	19 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Magnesic Red Kandosol Thin Non-gravelly Clay-loamy	Principal Profile Form:	Gn2.11
	 Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subrounded tabular, 
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	A1	0.03 - 0.08 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Moderate grade of structure, <2 mm, Granular; 
	5-10 mm, Polyhedral; Rough-ped fabric; Moist; Weak consistence; Field pH 5 (Raupach); Many, 
	very fine (0-1mm) roots; Common, fine (1-2mm) roots; Few, medium (2-5mm) roots; Clear, 
	Smooth change to - 
	B1	0.08 - 0.24 m	Dark reddish brown (5YR3/3-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 mm, 
	Polyhedral; 10-20 mm, Subangular blocky; Rough-ped fabric; Moist; Firm consistence; Field pH 
	2 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Common, medium (2-
	5mm) roots; Few, coarse (>5mm) roots; Gradual, Smooth change to - 
	B21	0.24 - 0.52 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Rough-ped fabric; Moist; Weak consistence; Field pH 5 (Raupach); 
	Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Few, medium (2-5mm) roots; 
	Few, coarse (>5mm) roots; Diffuse, Smooth change to - 
	B22	0.52 - 0.8 m	Dark reddish brown (2.5YR3/4-Moist); ; Light medium clay; Massive grade of structure; Earthy 
	fabric; Moist; Weak consistence; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; Few, fine 
	(1-2mm) roots; Few, medium (2-5mm) roots; Clear, Irregular change to - 
	B23	0.8 - 1.43 m	Red (2.5YR4/6-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; Moist; 
	Weak consistence; 10-20%, medium gravelly, 6-20mm, subangular, coarse fragments; Field pH 
	5.5 (Raupach); Clear change to - 
	B3	1.43 - 1.73 m	Yellowish brown (10YR5/6-Moist); ; Coarse sandy loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moist; Very weak consistence; Field pH 5.5 (Raupach); Gradual 
	change to - 
	C	1.73 - 2.83 m	Light olive brown (2.5Y5/4-Moist); ; Clayey coarse sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; Very weak consistence; Field pH 6 (Raupach); 
	Morphological Notes
	B23	Abrupt increase in gravel. This gravel  decreases in layer below.                                       
	                                                                                                
	Observation Notes

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site on slope above Paddys River. Downslope 50m is Hume and Hovell track. Granodiorite PM with fine grain material with 
	hornblende phenocrysts at 90cm.
	Site Notes
	COMP 85H 45738-3 17D 640M FROM BM099  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.03 - 0.08	4.08C	0.26H	0.13	0.21	0.01	2.09J	2.7E
	0K
	0.08 - 0.24	4.02C	0H	0.44	0.45	0.02	4.24J	5.15E
	0K
	0.24 - 0.52	4.02C	0H	1	0.64	0.07	4.3J	6E
	0K
	0.52 - 0.8	4.01C	0H	0.84	0.59	0.01	4.59J	6.02E
	0K
	0.8 - 1.43	4.02C	0H	0.43	0.42	0	3.12J	3.98E
	0K
	1.43 - 1.73	4.16C	0H	0.14	0.13	0.03	1.07J	1.36E
	0K
	1.73 - 2.83	4.28C	0H	0.15	0.07	0.01	0.57J	0.8E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.08	4.09B	384.9B	0.17A	0.95	31.86
	0.08 - 0.24	1.4B	243.9B	0.06A	1.13	24.54
	0.24 - 0.52	0.91B	446B	0.06A	1.05	24.33
	0.52 - 0.8	0.73B	343.7B	0.05A	1.27	23.25
	0.8 - 1.43	0.16B	301.7B	0.02A	20.76
	1.43 - 1.73	0.07B	279.7B	0A	4.44
	1.73 - 2.83	0.09B	435.8B	0.01A	5.31
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.08
	0.08 - 0.24
	0.24 - 0.52
	0.52 - 0.8
	0.8 - 1.43
	1.43 - 1.73
	1.73 - 2.83

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0100	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3