Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	06/05/96	Elevation:	1185 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6052206 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	606962  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Sgg	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Red Kandosol Medium Non-gravelly Silty 	Principal Profile Form:	Um6.
	Silty Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A1	0.02 - 0.16 m	Dark reddish brown (5YR3/3-Moist); ; Silty clay loam; Moderate grade of structure, 5-10 mm, 
	Polyhedral; Rough-ped fabric; Moist; Weak consistence; Many cutans, >50% of ped faces or 
	walls coated, faint; Field pH 6 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-2mm) 
	roots; Few, medium (2-5mm) roots; Clear, Smooth change to - 
	B21	0.16 - 0.44 m	Dark reddish brown (2.5YR3/4-Moist); Biological mixing, 2.5YR32, 2-10% , Distinct; Silty clay 
	loam; Moderate grade of structure, 10-20 mm, Polyhedral; 20-50 mm, Polyhedral; Rough-ped 
	fabric; Moist; Weak consistence; Common cutans, 10-50% of ped faces or walls coated, faint; 
	Field pH 6 (Raupach); Common, very fine (0-1mm) roots; Common, fine (1-2mm) roots; Few, 
	medium (2-5mm) roots; Few, coarse (>5mm) roots; Gradual, Smooth change to - 
	B22	0.44 - 0.77 m	Reddish brown (2.5YR4/4-Moist); Biological mixing, 5YR32, 2-10% , Distinct; Silty clay loam; 
	Weak grade of structure, 20-50 mm, Polyhedral; Earthy fabric; Moist; Weak consistence; Few 
	cutans, <10% of ped faces or walls coated, faint; Field pH 5.5 (Raupach); Common, very fine (0-
	1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Gradual, Smooth change to - 
	B23	0.77 - 1.57 m	Red (2.5YR4/6-Moist); ; Silty clay loam; Weak grade of structure, 20-50 mm, Polyhedral; Earthy 
	fabric; Moderately moist; Firm consistence; Few cutans, <10% of ped faces or walls coated, 
	faint; Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, 
	medium (2-5mm) roots; Abrupt, Smooth change to - 
	C1	1.57 - 2.32 m	Light yellowish brown (10YR6/4-Moist); ; Sandy loam; Massive grade of structure; Moderately 
	moist; Very weak consistence; Field pH 5.5 (Raupach); Diffuse, Smooth change to - 
	C2	2.42 - 3.02 m	Light yellowish brown (10YR6/4-Moist); Substrate influence, 10YR44, 20-50% , Faint; Sandy 
	loam; Massive grade of structure; Moderately moist; Very weak consistence; Field pH 5.5 
	(Raupach); 
	Morphological Notes
	A1	Not a particularly dark or organic A1 but abundant large (8mm) pores caused by stubby 
	worms.
	B21	Typical polyhedral structure associated with worm activity.                                                

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B22	"Blind crickets" colony at 65 -75cm. Density increasing and pedality declining.
	B23	Relatively dense and earthy B23. Mica flakes evident in earthy matrix.
	C1	Very sharp contrast with solum. C horizons have abundant mafic minerals and sandy 
	texture.
	C2	Very similar to 5 but may be more mafic minerals.                                                              
	                                                                                         
	Observation Notes
	Site is not far from outcropping granodiorite. Solum transition to C is very sharp. Snow gums and Mt. gums and cool elevated 
	Site Notes
	COMP 35H 16793-1 30.5D 275M FR INTER  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.16	4.2C	2.27H	1.16	0.79	0.07	4.78J	9.07E
	0K
	0.16 - 0.44	4.11C	0.55H	0.85	0.65	0.03	4.33J	6.42E
	0K
	0.44 - 0.77	3.98C	0.82H	0.67	0.54	0.08	4J	6.11E
	0K
	0.77 - 1.57	3.96C	0.05H	0.39	0.61	0.07	4.45J	5.57E
	0K
	1.57 - 2.32	4.13C	0.09H	0.09	0.27	0.04	1.06J	1.55E
	0K
	2.42 - 3.02	4.13C	0.11H	0.08	0.15	0.04	1.01J	1.4E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.16	4.08B	446.4B	0.22A	1.03	9.65
	0.16 - 0.44	1.9B	376B	0.12A	1.06	4.84
	0.44 - 0.77	0.75B	379.8B	0.06A	1.09	0
	0.77 - 1.57	0.26B	297.2B	0.04A	1.38	4.92
	1.57 - 2.32	0.09B	282.4B	0.01A	6.43
	2.42 - 3.02	0.04B	240.4B	0.01A	7.54
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.16
	0.16 - 0.44
	0.44 - 0.77
	0.77 - 1.57
	1.57 - 2.32
	2.42 - 3.02

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0119	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3