Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	N.J. McKenzie	Locality:
	Date Desc.:	07/05/96	Elevation:	1168 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6047079 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	604613  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	No Data	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	3 % 	Aspect:	135 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic-Mottled Dystrophic Grey Kandosol Medium Non-	Principal Profile Form:	Um6.14
	gravelly Silty Silty Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.01 m	Organic Layer; ; 
	A1	0.01 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Silty clay loam; Moderate grade of structure, 10-20 
	mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; Common cutans, 10-
	50% of ped faces or walls coated, faint; Field pH 4.5 (Raupach); Common, very fine (0-1mm) 
	roots; Common, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse (>5mm) roots; 
	Clear, Smooth change to - 
	B1	0.11 - 0.33 m	Yellowish brown (10YR5/4-Moist); Biological mixing, 10YR32, 20-50% , Distinct; Silty clay 
	loam; Moderate grade of structure, 10-20 mm, Polyhedral; Rough-ped fabric; Moist; Weak 
	consistence; 0-2%, coarse gravelly, 20-60mm, subangular platy, dispersed, Quartz, coarse 
	fragments; Few cutans, <10% of ped faces or walls coated, faint; Field pH 5 (Raupach); Many, 
	very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Clear, Smooth change to - 
	B2	0.33 - 0.61 m	Light brownish grey (10YR6/2-Moist); Substrate influence, 7.5YR58, 20-50% , Faint; Biological 
	mixing, 10YR32, 2-10% , Distinct; Medium sandy clay loam; Massive grade of structure; Earthy 
	fabric; Moist; Weak consistence; Few cutans, <10% of ped faces or walls coated, faint; Field 
	pH 5.5 (Raupach); Many, very fine (0-1mm) roots; Clear, Wavy change to - 
	C1	0.61 - 1.36 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR82, 20-50% , Distinct; Substrate influence, 
	7.5YR58, 10-20% , Prominent; Sandy loam; Massive grade of structure; Moist; Weak 
	consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), Soft segregations, weak, 
	segregations;Field pH 5.5 (Raupach); Few, very fine (0-1mm) roots; Diffuse, Smooth change to - 
	C2	1.36 - 2.26 m	Brownish yellow (10YR6/6-Moist); Substrate influence, 7.5YR68, 10-20% , Distinct; Mottles, 
	10YR82, 10-20% , Distinct; Medium sandy clay loam; Massive grade of structure; Wet; Weak 
	consistence; Field pH 5 (Raupach); Gradual, Smooth change to - 
	C3	2.26 - 2.86 m	Yellowish brown (10YR5/6-Moist); Substrate influence, 10YR64, 10-20% , Distinct; Medium 
	sandy clay loam; Massive grade of structure; Wet; Weak consistence; Field pH 5 (Raupach); 
	Morphological Notes
	A1	Moderate structure in A1 with much worm activity.                                                               

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	B1	Large worm channels backfilled with A1. Moderate structure os due to worms. Very pale 
	yellow most iron is Fe2+ or gone.
	B2	Pale yellow earthy B2.                                                                                                          
	                                                                        
	C1	C horizon has some Fe staining but most has been removed saprolite rather than  
	tranported colluvium.                                                                                                   
	C2	Yellowing and iron still in situ with micas and mafic minerals evident.
	C3	Similar to layer  5 but stonger yellowing.
	Observation Notes
	Site Notes
	COMP 72H 4179-1 90M FR/SADDLE 182DEG  

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01
	0.01 - 0.15	3.93C	1.48H	0.7	0.61	0.06	4.64J	7.49E
	0K
	0.11 - 0.33	3.99C	0.05H	0.17	0.16	0.07	2.47J	2.91E
	0K
	0.33 - 0.61	4C	0.05H	0.14	0.19	0.03	1.89J	2.3E
	0K
	0.61 - 1.36	4.03C	0.07H	0.09	0.12	0.03	1.79J	2.1E
	0K
	1.36 - 2.26	3.91C	0.07H	0.1	0.15	0.04	2.18J	2.54E
	0K
	2.26 - 2.86	3.9C	5.2H	2.28	0.42	0.13	5.5J	13.53E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.01 - 0.15	4.57B	393.2B	0.24A	0.86	8.54
	0.11 - 0.33	1.12B	206.4B	0.09A	1.08	7.43
	0.33 - 0.61	0.31B	130.3B	0.02A	1.40	5.22
	0.61 - 1.36	0.31B	117.1B	0.03A	1.27	7.22
	1.36 - 2.26	0.08B	105.9B	0.01A	5.99
	2.26 - 2.86	0.07B	149.8B	0.01A	6.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.15
	0.11 - 0.33
	0.33 - 0.61
	0.61 - 1.36
	1.36 - 2.26
	2.26 - 2.86

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0121	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3