Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0136	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	17/05/96	Elevation:	541 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6060549 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	614257  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Os	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	46 % 	Aspect:	45 degrees
	Surface Soil Condition (dry):
	Erosion:	Partial, Minor (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic  Orthic Tenosol Thin Moderately gravelly Loamy Clayey	Principal Profile Form:	Gn4.31
	 Moderately deep
	ASC Confidence:	Great Soil Group:	Brown earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subangular tabular, Schist; 20-50%, medium gravelly, 6-20mm, subangular platy, Schist; 
	20-50%, coarse gravelly, 20-60mm, subangular platy, Schist
	Profile Morphology
	O1	0 - 0.06 m	Organic Layer; ; 
	A1	0.06 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; Weak grade of structure, <2 mm, Granular; 
	Rough-ped fabric; Moderately moist; Loose consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular tabular, Schist, coarse fragments; Field pH 5.5 (Raupach); Abrupt, Smooth change 
	to - 
	A2	0.08 - 0.25 m	Yellowish brown (10YR5/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, subangular tabular, Schist, 
	coarse fragments; Field pH 5 (Raupach); Many, very fine (0-1mm) roots; Many, fine (1-2mm) 
	roots; Common, medium (2-5mm) roots; Clear, Irregular change to - 
	B2	0.25 - 0.42 m	Strong brown (7.5YR4/6-Moist); ; Light medium clay; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Rough-ped fabric; Moderately moist; Weak consistence; 50-90%, fine 
	gravelly, 2-6mm, subangular tabular, Schist, coarse fragments; Field pH 5 (Raupach); Common,
	 very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) roots; Few, coarse 
	(>5mm) roots; Gradual, Irregular change to - 
	BC	0.42 - 0.69 m	Strong brown (7.5YR4/6-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; 
	Moderately moist; Firm consistence; 50-90%, medium gravelly, 6-20mm, subangular tabular, 
	Schist, coarse fragments; Field pH 5 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm)
	 roots; Clear, Irregular change to - 
	Morphological Notes
	A1	No root abundance measures due to thinness. Steep slopes and frequent fire regime 
	has stripped this layer.
	A2	Several patches of fungal hyphae producing hydrophobic soil.
	B2	Increasing gravel.                                                                                                                 
	                                                                     
	BC	Increase in situ gravel.                                                                                                         
	                                                                       
	Observation Notes
	A steep exposed slope. Last fire >20yrs. Almost pure stringybark.                                                                                                    

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0136	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Notes
	COMP 121H 898-1 90D 320M FROM 876-1   

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0136	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06
	0.06 - 0.08	3.45C	2.31H	0.93	1.06	0.12	7.06J	15.58E
	4.1K
	0.08 - 0.25	3.86C	0.13H	0.2	0.68	0.1	3.6J	4.72E
	0K
	0.25 - 0.42	3.97C	0.11H	0.23	0.67	0.08	3.4J	4.5E
	0K
	0.42 - 0.69	3.98C	0.04H	0.22	0.49	0.08	1.98J	2.81E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.06 - 0.08	12.44B	263.7B	0.4A	0.80	11.88
	0.08 - 0.25	3.02B	176.8B	0.11A	42.39
	0.25 - 0.42	1.74B	209B	0.1A	52.45
	0.42 - 0.69	0.43B	308.6B	0.07A	53.47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.08
	0.08 - 0.25
	0.25 - 0.42
	0.42 - 0.69

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0136	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3