Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	23/05/96	Elevation:	573 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6061448 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	614650  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Os	Substrate Material:	Schist 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	60 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):
	Erosion:	Minor (sheet) Active, Present (mass) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic  Orthic Tenosol Thin Moderately gravelly Clay-loamy 	Principal Profile Form:	Gn4.11
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable group
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, subangular platy, ; 20-50%, medium gravelly, 6-20mm, subangular platy, ; 20-50%, fine 
	gravelly, 2-6mm, angular tabular, Coal
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; ; 
	A1	0.02 - 0.08 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy clay loam; Weak grade of structure, <2 mm, Granular; 
	Rough-ped fabric; Moderately moist; Very weak consistence; 20-50%, fine gravelly, 2-6mm, 
	subangular tabular, coarse fragments; Field pH 4 (Raupach); Many, very fine (0-1mm) roots; 
	Common, fine (1-2mm) roots; Common, medium (2-5mm) roots; Clear, Irregular change to - 
	B21	0.08 - 0.27 m	Reddish brown (5YR4/4-Moist); Biological mixing, 7.5YR2.52, 2-10% , Faint; Clay loam; Weak 
	grade of structure, 2-5 mm, Polyhedral; 10-20 mm, Subangular blocky; Rough-ped fabric; 
	Moderately moist; Weak consistence; 20-50%, fine gravelly, 2-6mm, subangular tabular, coarse 
	fragments; Field pH 5.5 (Raupach); Common, very fine (0-1mm) roots; Common, fine (1-2mm) 
	roots; Common, medium (2-5mm) roots; Gradual, Irregular change to - 
	B22	0.27 - 0.5 m	Dark reddish brown (5YR3/4-Moist); Biological mixing, 2-10% , Distinct; Clay loam; Weak grade 
	of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Moist; Weak consistence; 20-50%, 
	fine gravelly, 2-6mm, subangular tabular, coarse fragments; Few cutans, <10% of ped faces or 
	walls coated, faint; Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Common, fine (1-
	2mm) roots; Few, medium (2-5mm) roots; Gradual, Irregular change to - 
	BC	0.5 - 0.72 m	Yellowish red (5YR4/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Moist; Weak
	 consistence; 50-90%, coarse gravelly, 20-60mm, subangular tabular, coarse fragments; Field 
	pH 4 (Raupach); Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Gradual, Irregular change
	 to - 
	Morphological Notes
	A1	Layers 1 to 3 have a colluvial origin.                                                                                    
	                                                                              
	B21	Large pores/burrows due to blind crickets.
	Observation Notes
	Very steep slope - loose gravel, soil and litter produce numerous terracettes. Active colluvial slope movement.
	Site Notes
	COMP 121H 468-1 172D 160M FROM RD BND 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02
	0.02 - 0.08	4.06C	4.88H	1.61	0.79	0.08	6.32J	14.23E
	0.56K
	0.08 - 0.27	4.29C	0.65H	0.74	0.55	0.05	2.5J	4.49E
	0K
	0.27 - 0.5	4.17C	0.12H	0.97	0.55	0.06	3.31J	5E
	0K
	0.5 - 0.72	4.06C	0.16H	0.77	0.55	0.04	2.68J	4.2E
	0K
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02
	0.02 - 0.08	10.17B	505.7B	0.3A	0.85	62.6
	0.08 - 0.27	2.45B	373.7B	0.11A	0.97	53.25
	0.27 - 0.5	2.93B	327.4B	0.09A	39.8
	0.5 - 0.72	0.6B	333.6B	0.06A	34.49
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.08
	0.08 - 0.27
	0.27 - 0.5
	0.5 - 0.72

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3