Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0156	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P. Ryan	Locality:
	Date Desc.:	08/04/97	Elevation:	1114 metres
	Map Ref.:	Sheet No. : 8526   DGPS	Rainfall:	No Data
	Northing/Long.:	6042227 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	603869  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Tb	Substrate Material:	Granodiorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	0 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Kandosolic Redoxic Hydrosol Medium Non-gravelly 	Principal Profile Form:	Uf3.
	Silty Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Wiesenboden
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; ; 
	A11	0.03 - 0.12 m	Very dark brown (10YR2/2-Moist); ; Silty clay loam; Moderate grade of structure, 10-20 mm, 
	Angular blocky; 5-10 mm, Polyhedral; Rough-ped fabric; Moderately moist; Firm consistence; 
	10-20%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, 
	Fine (0 - 2 mm), Root linings; Field pH 4.5 (Raupach); Many, very fine (0-1mm) roots; Common, 
	fine (1-2mm) roots; Clear change to - 
	A12	0.12 - 0.21 m	Very dark grey (10YR3/1-Moist); ; Silty clay loam; Moderate grade of structure, 10-20 mm, 
	Angular blocky; 5-10 mm, Polyhedral; Smooth-ped fabric; Moderately moist; Firm consistence; 
	2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few cutans, <10% of ped faces 
	or walls coated; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Root linings; Field pH 4.5 
	(Raupach); Common, very fine (0-1mm) roots; Few, fine (1-2mm) roots; Few, medium (2-5mm) 
	roots; Clear change to - 
	A2	0.21 - 0.39 m	Brown (10YR5/3-Moist); Substrate influence, 10YR56, 2-10% , Faint; Silty clay; Massive grade of
	 structure; Earthy fabric; Moderately moist; Weak consistence; Field pH 4 (Raupach); Few, very 
	fine (0-1mm) roots; Few, fine (1-2mm) roots; Clear change to - 
	B2	0.39 - 0.68 m	Yellowish brown (10YR5/6-Moist); Substrate influence, 10YR53, 10-20% , Faint; Silty clay; 
	Massive grade of structure; Earthy fabric; Moist; Weak consistence; 2-10%, fine gravelly, 2-6mm,
	 subangular, Quartz, coarse fragments; Few cutans, <10% of ped faces or walls coated, faint; 
	Field pH 4.5 (Raupach); Few, very fine (0-1mm) roots; Clear change to - 
	C11	0.68 - 0.98 m	Grey (10YR6/1-Moist); Substrate influence, 10YR56, 0-2% , Faint; Medium sandy clay loam; 
	Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak consistence; 2-10%, 
	fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Field pH 5 (Raupach); Few, very fine
	 (0-1mm) roots; Clear change to - 
	C12	0.98 - 1.58 m	Light brownish grey (2.5Y6/2-Moist); Substrate influence, 10YR56, 2-10% , Faint; Medium sandy 
	clay loam; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; Field pH 5.5 (Raupach); Gradual change to - 
	C2	1.58 - 2.28 m	; Coarse sandy loam; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; Field pH 6 (Raupach); Clear change to - 

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0156	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	C3	2.28 - 3.63 m	; Coarse sandy loam; Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; Field pH 7 (Raupach); 
	Morphological Notes
	A11	Organic rich. Basalt colluvium?                                                                                           
	                                                                              
	A2	Pale A2 horizon.                                                                                                                   
	                                                                     
	B2	Muscovite and quartz in sand fraction.                                                                                 
	                                                                                 
	C11	At top of layer there is a layer of 2-6mm quartz gravel. Remainder of layer is pale 
	weathered granodiorite. Muscovite rich, quartz poor.
	C12	Weathering granodiorite with some brown mottling. Muscovite rich, quartz poor.                
	                                                                                                          
	C2	Less weathered granodiorite, sandy with  banded Fe-stained areas.
	C3	Weathered granodiorite - no Fe-staining                                                                              
	                                                                                   
	Observation Notes
	Site is in a broad drainage line supposedly with basalt on either side. A surprising shallow profile with little influence of basalt.
	Site Notes
	BURRA RD, HEAD OF MCCABES GULLY       

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0156	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03
	0.03 - 0.12	4.14C	2.57H	0.91	0.97	0	5.95J	10.4E
	0K
	0.12 - 0.21	4.05C	1.04H	0.53	0.78	0	6.13J	8.49E
	0K
	0.21 - 0.39	4.1C	0.94H	0.84	0.5	0	3.43J	5.71E
	0K
	0.39 - 0.68	4.31C	1.19H	2.18	0.13	0	1.85J	5.35E
	0K
	0.68 - 0.98	4.33C	0.63H	1.89	0.08	0.01	1.23J	3.83E
	0K
	0.98 - 1.58	4.35C	0.65H	2.03	0.12	0	1.01J	3.81E
	0K
	1.58 - 2.28
	2.28 - 3.63
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.12	5.07B	1072.1B	0.39A	0.81	5.68
	0.12 - 0.21	2.5B	560.1B	0.18A	0.96	4.4
	0.21 - 0.39	0.94B	287.7B	0.08A	1.26	6.28
	0.39 - 0.68	0.57B	319.5B	0.05A	1.38	14.71
	0.68 - 0.98	0.14B	352.3B	0.02A	5.07
	0.98 - 1.58	0.11B	314.4B	0.01A	7.87
	1.58 - 2.28	8
	2.28 - 3.63	8.36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.12
	0.12 - 0.21
	0.21 - 0.39
	0.39 - 0.68
	0.68 - 0.98
	0.98 - 1.58
	1.58 - 2.28
	2.28 - 3.63

	Project Name:	BAGO-MARAGLE FOREST SOIL SURVEY         
	Project Code:	BGM_FSS	Site ID:	0156	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	13C1_AL	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_H	Exchangeable H - by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	2A1	Air-dry moisture content
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3