Project Name:	CAN
	Project Code:	CAN	Site ID:	CP143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	P.H. Walker	Locality:
	Date Desc.:	31/05/79	Elevation:	 580 metres
	Map Ref.:	Sheet No. : S1 55-16   1:250000	Rainfall:	640
	Northing/Long.:	149.183333333333	Runoff:	Very slow
	Easting/Lat.:	-35.3388888888889	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Porous, Unconsolidated material 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	290 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.1
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Sod grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.17 m	Dark red (2.5YR3/6-Moist); ; Fine sandy loam; Massive grade of structure; Firm consistence; 
	Clear change to - 
	A2	0.17 - 0.3 m	Dark red (2.5YR3/6-Moist); ; Fine sandy loam; Massive grade of structure; Firm consistence; 
	Diffuse change to - 
	B1	0.3 - 0.45 m	Dark red (2.5YR3/6-Moist); ; Clay loam, fine sandy; Massive grade of structure; Firm 
	consistence; Diffuse change to - 
	B1	0.45 - 0.6 m	Dark red (2.5YR3/6-Moist); ; Clay loam, fine sandy; Massive grade of structure; Very firm 
	consistence; 
	B21	0.6 - 0.9 m	Dark red (10R3/6-Moist); ; Light clay; Massive grade of structure; Very strong consistence; 
	Diffuse change to - 
	B22	0.9 - 1.2 m	Dark red (10R3/6-Moist); ; Light clay; Massive grade of structure; Very strong consistence; 
	Diffuse change to - 
	Morphological Notes
	Observation Notes
	APPROX. 10CM OVERBURDEN REMOVED:CAINOZOIC ALLUVIUM (MOLONGOLO RV.)                                                      
	Site Notes
	FYSHWICK/Q'BYN

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	CAN
	Project Code:	CAN	Site ID:	CP143	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile