Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Coolamon, NSW.  Owner M Willis
	Date Desc.:	01/01/78	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	147.33333333	Runoff:	No Data
	Easting/Lat.:	-34.9	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.11
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.09 m	Dark reddish brown (5YR3/3-Moist); ; Loam; Massive grade of structure; Weak consistence; 
	Field pH 5 (Raupach); 
	0.09 - 0.2 m	Dark red (2.5YR3/5-Moist); ; Clay loam; Massive grade of structure; Weak consistence; 
	0.2 - 0.5 m	Dark red (2.5YR3/8-Moist); ; Light clay; Weak grade of structure, Angular blocky; Firm 
	consistence; 
	0.5 - 1 m	Strong brown (7.5YR5/6-Moist); ; Light clay; Weak grade of structure, Angular blocky; Firm 
	consistence; Field pH 6 (Raupach); 
	Morphological Notes
	Observation Notes
	Met Stn:  Soil Con Stn.  Rain zone Wm
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7A	0.1A
	0.02 - 0.07
	0.1 - 0.2	5.6A	0.06A
	0.2 - 0.3	6.3A	0.05A
	0.3 - 0.4	6.6A	0.04A
	0.4 - 0.6	7A	0.05A
	0.6 - 0.8	6.3A	0.06A
	0.75 - 0.8
	0.8 - 1	6.3A	0.06A
	1 - 1.2	7.9A	0.04A
	1.2 - 1.6	8.6A	0.04A
	1.6 - 2	8.7A	0.07A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0C	1.46A	9A	52	15	21
	0.02 - 0.07	1.36
	0.1 - 0.2	0C	0.59A	8A	46	16	29
	0.2 - 0.3	0C	0.33A	9A	42	13	35
	0.3 - 0.4	0C	0.28A	9A	40	12	39
	0.4 - 0.6
	0.6 - 0.8
	0.75 - 0.8	1.63
	0.8 - 1
	1 - 1.2	0.03C	6A	32	12	48
	1.2 - 1.6	0.04C	7A	33	12	44
	1.6 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.02 - 0.07	0.42D	0.31D	0.29D	0.2D	0.12E	97.08333C
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.8
	0.75 - 0.8	0.36D	0.32D	0.31D	0.26D	0.19E	8.333333C
	0.8 - 1
	1 - 1.2
	1.2 - 1.6
	1.6 - 2

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B1VL_1	1 BAR Moisture m3/m3 - Volumetric using <2mm sample on pressure plate
	P3B1VL_15	15 BAR Moisture m3/m3 - Volumetric using <2mm sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)