Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Roseworthy, SA.  Ag College E13
	Date Desc.:	01/01/79	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	138.73333333	Runoff:	No Data
	Easting/Lat.:	-34.5	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gc1.11
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Confidence level not specified	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.18 m	; Loam (Light); Massive grade of structure; Weak consistence; Field pH 8 (Raupach); 
	0.18 - 0.79 m	; Clay loam (Light); Massive grade of structure; Firm consistence; Field pH 8.5 (Raupach); 
	0.79 - 1.2 m	; Light medium clay; Weak grade of structure, Prismatic; Very firm consistence; Field pH 9 
	(Raupach); 
	Morphological Notes
	Carbonate from surface becoming CO3 free with depth
	Observation Notes
	Met Stn:  on site.  Rain zone Wl
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.1A	0.21A
	0.1 - 0.2	8.4A	0.16A
	0.1 - 0.15
	0.2 - 0.3	8.4A	0.17A
	0.3 - 0.5	8.9A	0.18A
	0.35 - 0.4
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3	9.3A	0.91A
	1.3 - 1.7
	1.7 - 2.1	7.1A	1.14A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	3.5C	1.56A	16A	51	8	20
	0.1 - 0.2	16.7C	0.89A	16A	42	7	18
	0.1 - 0.15	1.59
	0.2 - 0.3	0.57A
	0.3 - 0.5	44.8C	0.35A	10A	25	2	17
	0.35 - 0.4	1.26
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1	0.09C	12A	38	7	48
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.1 - 0.15	0.34D	0.3D	0.28D	0.19E	0.16F	6.666667C
	0.2 - 0.3
	0.3 - 0.5
	0.35 - 0.4	0.45D	0.37D	0.32D	0.21E	0.15F	16.25C
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)