Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Turretfield, SA. Ag Res Stn
	Date Desc.:	01/01/79	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	138.86666666	Runoff:	No Data
	Easting/Lat.:	-34.55	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr2.23
	ASC Confidence:	Great Soil Group:	Red-brown earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Massive grade of structure; Firm consistence; 
	Field pH 7.5 (Raupach); 
	A2	0.1 - 0.13 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Field pH 8 
	(Raupach); 
	B1	0.13 - 0.52 m	Dark reddish brown (2.5YR3/3-Moist); ; Medium clay; Strong grade of structure, Prismatic; Very 
	firm consistence; Field pH 8.5 (Raupach); 
	B2	0.52 - 1.2 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium clay; Strong grade of structure, Prismatic; Field 
	pH 9.5 (Raupach); 
	Morphological Notes
	B1	Carbonate from 46cms
	Observation Notes
	Met St:  on site  Rain zone Wl
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.3A	0.11A
	0.03 - 0.08
	0.1 - 0.2	7.1A	0.13A
	0.2 - 0.3	7.6A	0.24A
	0.25 - 0.3
	0.3 - 0.5	8.7A	0.41A
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3	9.1A	0.62A
	1.3 - 1.7
	1.7 - 2.1	9.1A	0.65A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.47A	5A	54	26	15
	0.03 - 0.08	1.50
	0.1 - 0.2	0.82A	3A	39	28	33
	0.2 - 0.3	0.7A
	0.25 - 0.3	1.21
	0.3 - 0.5	3.59C	0.43A	1A	14	12	71
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1	24.8C	2A	15	8	52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.03 - 0.08	0.4D	0.34D	0.32D	0.24E	0.1F	19.58333C
	0.1 - 0.2
	0.2 - 0.3
	0.25 - 0.3	0.51D	0.5D	0.46E	0.35F	4.166667E-
	02C
	0.3 - 0.5
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	37	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)