Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	43	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Cowra, NSW.  Owner H Wright
	Date Desc.:	01/01/79	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	148.81666666	Runoff:	No Data
	Easting/Lat.:	-33.81666666	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Weak 
	consistence; Field pH 4.5 (Raupach); 
	A2	0.1 - 0.37 m	Reddish yellow (5YR6/6-Moist); ; Sandy loam; Massive grade of structure; Weak consistence; 
	Field pH 5.5 (Raupach); 
	B1	0.37 - 0.5 m	Red (2.5YR5/6-Moist); ; Medium clay; , Angular blocky; Very firm consistence; Field pH 7 
	(Raupach); 
	B2	0.5 - 0.9 m	Reddish brown (2.5YR5/4-Moist); ; Heavy clay; , Angular blocky; Very firm consistence; Field pH 
	8 (Raupach); 
	Morphological Notes
	Observation Notes
	Met Stn:  Soil Con Stn.  Rain zone Um
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	43	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.3A	0.08A
	0.08 - 0.13
	0.1 - 0.2	5A	0.06A
	0.2 - 0.3
	0.3 - 0.5	6.8A	0.04A
	0.36 - 0.41
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1	8A	0.09A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0C	0.65A	30A	49	14	6
	0.08 - 0.13	1.53
	0.1 - 0.2	0C	0.57A	29A	50	14	7
	0.2 - 0.3
	0.3 - 0.5	0C	0.19A	17A	26	8	51
	0.36 - 0.41	1.42
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1	0.13C	15A	36	13	37
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.08 - 0.13	0.41D	0.33D	0.3D	0.11E	0.06F	12.91667C
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.36 - 0.41	0.46D	0.39D	0.37D	0.3E	0.24F	45.83334C
	0.5 - 0.7
	0.7 - 0.9
	0.9 - 1.3
	1.3 - 1.7
	1.7 - 2.1

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	43	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)