Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Horsham, Vic.  Owner - D.Ladlow
	Date Desc.:	01/01/78	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	142.25	Runoff:	No Data
	Easting/Lat.:	-36.6	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug5.16
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.8 m	Very dark greyish brown (10YR3/2-Moist); ; Light clay; , Prismatic; Smooth-ped fabric; Firm 
	consistence; Field pH 8.5 (Raupach); 
	0.8 - 2 m	; Light medium clay; , Prismatic; Smooth-ped fabric; Firm consistence; Field pH 9 (Raupach); 
	Morphological Notes
	Carbonate from surface
	Observation Notes
	Met station - Longerenong.  Rain zone Wl
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.1A	0.28A
	0.05 - 0.1
	0.1 - 0.2	8.3A	0.29A
	0.2 - 0.3	8.5A	0.34A
	0.3 - 0.4	8.8A	0.43A
	0.3 - 0.35
	0.4 - 0.6	9A	0.59A
	0.6 - 0.8	9.1A	0.95A
	0.8 - 1	9A	1.3A
	1 - 1.2	9A	1.5A
	1.2 - 1.6	9A	2A
	1.6 - 2	8.9A	2.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	3.9C	0.87A	13A	15	15	49
	0.05 - 0.1	1.12
	0.1 - 0.2	4.1C	0.63A	11A	12	13	58
	0.2 - 0.3	4.6C	0.59A	11A	11	10	59
	0.3 - 0.4	4.9C	0.54A	10A	11	11	59
	0.3 - 0.35	1.09
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 1	7.8C	7A	9	11	62
	1 - 1.2
	1.2 - 1.6
	1.6 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.05 - 0.1	0.53D	0.47D	0.45D	0.41E	0.24F	4.166667C
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.3 - 0.35	0.59D	0.48D	0.46D	0.41E	0.31F	27.08333C
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2
	1.2 - 1.6
	1.6 - 2

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	5	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)