Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Locality:	Condobolin NSW.  Owner J Tunks
	Date Desc.:	01/01/78	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	147.08333333	Runoff:	No Data
	Easting/Lat.:	-32.98333333	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gn2.12
	ASC Confidence:	Great Soil Group:	Red earth
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark reddish brown (2.5YR3/4-Moist); ; Fine sandy loam; Massive grade of structure; Weak 
	consistence; Field pH 6 (Raupach); 
	0.08 - 0.67 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Weak consistence; 
	Field pH 5 (Raupach); 
	0.67 - 0.75 m	Dark red (2.5YR3/6-Moist); ; Sandy clay loam; Weak grade of structure, Prismatic; Firm 
	consistence; Field pH 6.5 (Raupach); 
	Morphological Notes
	Observation Notes
	Met station - Soil Con stn.  Rain zone U1
	Site Notes

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.3A	0.07A
	0.05 - 0.1
	0.1 - 0.2	4.8A	0.07A
	0.2 - 0.3	4.6A	0.07A
	0.3 - 0.4	4.6A	0.06A
	0.4 - 0.6	5A	0.06A
	0.6 - 0.8	6.3A	0.08A
	0.66 - 0.71
	0.8 - 1	7.7A	0.08A
	1 - 1.2	8.2A	0.08A
	1.2 - 1.6	8.5A	0.08A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0C	0.56A	39A	39	7	14
	0.05 - 0.1	1.63
	0.1 - 0.2	0C	0.41A	34A	39	8	21
	0.2 - 0.3	0C	0.36A	33A	38	8	20
	0.3 - 0.4	0C	0.25A	33A	38	7	21
	0.4 - 0.6	0C	0.17A	32A	39	7	22
	0.6 - 0.8	0C	0.15A	26A	39	8	28
	0.66 - 0.71	1.73
	0.8 - 1
	1 - 1.2
	1.2 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.05 - 0.1	0.3D	0.21D	0.18D	0.13E	0.09F	40.83334C
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.6
	0.6 - 0.8
	0.66 - 0.71	0.29D	0.24D	0.23D	0.21E	0.18F	10C
	0.8 - 1
	1 - 1.2
	1.2 - 1.6

	Project Name:	Wheatland Soils in Eastern Australia
	Project Code:	Forrest	Site ID:	7	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P3A1	Bulk density - g/cm3
	P3B2VL_1	1 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B2VL_15	15 BAR Moisture m3/m3 - Volumetric using disturbed sample on pressure plate
	P3B3VLa005	0.05 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLa01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P3B3VLaSAT	Saturated Moisture m3/m3 - Volumetric using undisturbed 76mm diameter core on suction plate
	P4_sat_For	Saturated Hydraulic Conductivity (Forrest et al, 1985)