Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:
	Date Desc.:	04/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 9033   1:100000	Rainfall:	No Data
	Northing/Long.:	150.86694444	Runoff:	No Data
	Easting/Lat.:	-32.14805556	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Black Vertosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Black earth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.1 m	Very dark brown (10YR2/2-Dry); ; Light medium clay; Strong consistence; Common, fine (1-
	2mm) roots; 
	A12	0.1 - 0.2 m	Very dark greyish brown (10YR3/2-Dry); ; Light medium clay; Weak consistence; Few, medium 
	(2-5mm) roots; 
	B2	0.2 - 0.4 m	Dark brown (10YR3/3-Dry); ; Light clay (Light); Weak consistence; Few, fine (1-2mm) roots; 
	2	0.4 - 1 m	Black (2.5Y2/0-Moist); ; Medium clay; Firm consistence; Few, very fine (0-1mm) roots; 
	Morphological Notes
	2	Black clay.
	Observation Notes
	Soil type: Prairee/Black earth?
	Site Notes
	James Birch.  Lucerne pasture.  Sandier site.

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.63D	0.152A	21H	15.1	0.34	0.9	37.35D
	0.1 - 0.2	7D	0.102A	23.41H	15.41	0.25	1.15	40.24D
	0.2 - 0.4	6.62D	0.101A	21.29H	13.76	0.21	1.24	36.52D
	0.5 - 0.7	7.11D	0.275A	30.19H	18	0.22	2.44	50.86D
	0.8 - 1	7.42D	0.401A	29.1H	26.21	0.22	5.12	60.66D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	3.13A	39J
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP343	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_AL	Exchangeable aluminium - method not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	3A1	EC of 1:5 soil/water extract
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9B1	Bicarbonate-extractable phosphorus - manual colour