Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP362	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:	Wynot.
	Date Desc.:	06/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 9033   1:100000	Rainfall:	No Data
	Northing/Long.:	150.67111111	Runoff:	No Data
	Easting/Lat.:	-32.32805556	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Steep low hills 30-90m 32-56%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Brown Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Greyish brown (10YR5/2-Dry); ; Loamy coarse sand; 0-2%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Common, fine (1-2mm) roots; Clear, Smooth change to - 
	A21	0.1 - 0.2 m	Very pale brown (10YR7/3-Dry); ; Loamy coarse sand; 0-2%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Few, very fine (0-1mm) roots; Gradual, Smooth change
	A22	0.2 - 0.7 m	Light yellowish brown (10YR6/4-Dry); ; Loamy coarse sand; 0-2%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; Clear, Smooth change to - 
	B2	0.7 - 1 m	Yellowish brown (10YR5/6-Dry); , 10YR63, 10-20% , 15-30mm, Prominent; Clay loam, coarse 
	sandy; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; 
	Morphological Notes
	A22	Partially cemented upper A2 at approximately 20 cm.
	Observation Notes
	Soil type: duplex soil , similar to CP361 but fewer stones.
	Site Notes
	Musswellbrook sheet.  River flat.  Tall grass pasture.

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP362	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.25D	0.044A	2.11H	0.86	0.46	0.13	3.66D
	0.1 - 0.2	5.42D	0.022A	1.49H	0.58	0.23	0.19	2.54D
	0.2 - 0.4	5.62D	0.057A	2.34H	2.6	0.31	0.94	6.22D
	0.5 - 0.7	6.35D	0.086A	1.29H	2.58	0.37	1.48	5.72D
	0.8 - 1	6.95D	0.152A	1.56H	3.45	0.45	2.11	7.57D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.55A	2J
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP362	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_AL	Exchangeable aluminium - method not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	3A1	EC of 1:5 soil/water extract
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9B1	Bicarbonate-extractable phosphorus - manual colour