Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP367	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:	Hebden/Mountain View.
	Date Desc.:	06/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 9133   1:100000	Rainfall:	No Data
	Northing/Long.:	151.04388889	Runoff:	No Data
	Easting/Lat.:	-32.34666667	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	100 metres
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	360 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Natric Grey Kurosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Loam; 2-10%, medium gravelly, 6-20mm, subangular, coarse 
	fragments; Many, fine (1-2mm) roots; Clear, Smooth change to - 
	A2	0.1 - 0.21 m	Pale brown (10YR6/3-Moist); ; Fine sandy loam (Light); 2-10%, medium gravelly, 6-20mm, 
	subangular, coarse fragments; Common, fine (1-2mm) roots; Abrupt, Wavy change to - 
	B2	0.21 - 0.7 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay; 0-2%, fine gravelly, 2-6mm, subangular, 
	coarse fragments; Few, very fine (0-1mm) roots; Gradual, Wavy change to - 
	C	0.7 - 1 m	Dark reddish grey (5YR4/2-Moist); , 7.5YR72, 10-20% , 5-15mm, Prominent; Sandy clay (Light); 
	10-20%, fine gravelly, 2-6mm, angular, coarse fragments; Few, very fine (0-1mm) roots; 
	Morphological Notes
	C	Mottle is probably due to rock fragments.
	Observation Notes
	Brown duplex soil.
	Site Notes
	Footslope, 200 metres to west of house.  Grassland including Themeda species.  Rosevale land system.

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP367	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.5D	0.044A	2.58H	1.48	0.71	0.23	5.52D
	0.1 - 0.2	4.78D	0.057A	2.04H	2.09	0.37	0.63	5.24D
	0.2 - 0.4	4.3D	0.174A	3.36H	8.42	0.35	3.1	15.97D
	0.5 - 0.7	4D	0.383A	3.54H	10.27	0.41	6.12	22.18D
	0.8 - 1	4D	0.446A	3.47H	11.93	0.33	7.25	24.89D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.38A	3J
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP367	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_AL	Exchangeable aluminium - method not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	3A1	EC of 1:5 soil/water extract
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9B1	Bicarbonate-extractable phosphorus - manual colour