Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:	Cessnock State Forest.
	Date Desc.:	08/04/93	Elevation:	5 metres
	Map Ref.:	Sheet No. : 9132   1:100000	Rainfall:	No Data
	Northing/Long.:	151.38194444	Runoff:	No Data
	Easting/Lat.:	-32.80805556	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Brown Kurosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Brown (10YR4/3-Dry); ; Loamy sand; 2-10%, medium gravelly, 6-20mm, coarse fragments; 
	Many, fine (1-2mm) roots; 
	A2	0.1 - 0.2 m	Pinkish grey (7.5YR7/2-Dry); ; Loamy sand; 2-10%, medium gravelly, 6-20mm, coarse 
	fragments; Many, medium (2-5mm) roots; 
	B21	0.2 - 0.5 m	Yellowish brown (10YR5/4-Dry); , 10YR58, 10-20% , 5-15mm, Faint; Medium clay; 0-2%, 
	medium gravelly, 6-20mm, rounded, Quartz, coarse fragments; Common, medium (2-5mm) roots; 
	BC	0.5 - 1 m	Light yellowish brown (10YR6/4-Dry); , 5YR56, 10-20% , 5-15mm, Distinct; , 10YR73; Light 
	clay; Few, very fine (0-1mm) roots; 
	Morphological Notes
	B21	Light Clay texture is sandy.
	Observation Notes
	Site Notes
	Spotted gums and ground cover.  Undulating low hills.

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.88D	0.065A	2.9H	1.87	0.39	0.25	5.73D
	0.1 - 0.2	4.48D	0.037A	0.21H	0.44	0.13	0.16	1.45D
	0.2 - 0.4	4.75D	0.342A	0.04H	8.61	0.24	2.84	12.06D
	0.5 - 0.7	5.02D	0.73A	0.14H	9.33	0.18	6.93	16.66D
	0.8 - 1	5.95D	0.903A	0.22H	11.44	0.28	8.06	20.02D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.93A	2J
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.5 - 0.7
	0.8 - 1

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP384	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_AL	Exchangeable aluminium - method not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	3A1	EC of 1:5 soil/water extract
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9B1	Bicarbonate-extractable phosphorus - manual colour