Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP389	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	C.J. Chartres	Locality:	Adhman's Brokerd.
	Date Desc.:	08/04/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 9132   1:100000	Rainfall:	No Data
	Northing/Long.:	151.27305556	Runoff:	No Data
	Easting/Lat.:	-32.76805556	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	1 % 	Aspect:	360 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Red Kurosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.2 m	Brown (10YR5/3-Dry); ; Fine sandy loam; Many, medium (2-5mm) roots; Gradual, Smooth 
	change to - 
	A2	0.2 - 0.3 m	Brown (10YR4/3-Dry); ; Sandy clay loam; Few, medium (2-5mm) roots; Abrupt, Irregular 
	change to - 
	B21	0.3 - 0.4 m	Brown (10YR4/3-Dry); ; Light medium clay; Few, medium (2-5mm) roots; Gradual, Smooth 
	change to - 
	B22	0.4 - 0.8 m	Light red (2.5YR6/6-Moist); , 10YR62, 10-20% , 5-15mm, Faint; Light medium clay; 2-10%, 
	coarse gravelly, 20-60mm, coarse fragments; Few, medium (2-5mm) roots; Clear, Irregular 
	change to - 
	BC	0.8 - 1 m	Dark greyish brown (10YR4/2-Moist); , 10YR58, 10-20% , 5-15mm, Faint; Sandy clay loam; 2-
	10%, coarse gravelly, 20-60mm, coarse fragments; Few, medium (2-5mm) roots; 
	Morphological Notes
	A2	Some zones A2 = 10YR6/2
	Observation Notes
	Yellowish duplex soil.
	Site Notes
	Tyrell's Vineyard.  Gently undulating.

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP389	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.98D	0.089A	5.03H	0.55	0.58	0.03	6.25D
	0.1 - 0.2	5.4D	0.085A	5.86H	0.74	0.51	0.12	7.3D
	0.2 - 0.4	5.2D	0.078A	4.59H	1.23	0.22	0.22	6.32D
	0.3 - 0.4	4.8D	0.088A	5.81H	3.21	0.34	0.31	9.85D
	0.5 - 0.7	5.2D	0.128A	5.53H	4.92	0.31	0.59	11.39D
	0.8 - 1	6.7D	0.093A	4.45H	4.14	0.22	1.53	10.37D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.05A	12J
	0.1 - 0.2
	0.2 - 0.4
	0.3 - 0.4
	0.5 - 0.7
	0.8 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.4
	0.3 - 0.4
	0.5 - 0.7
	0.8 - 1

	Project Name:	Hunter Valley Soil Survey
	Project Code:	HV	Site ID:	CP389	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_AL	Exchangeable aluminium - method not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	3A1	EC of 1:5 soil/water extract
	4C1	pH of 1:5 soil/1M potassium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9B1	Bicarbonate-extractable phosphorus - manual colour