Project Name:	Irrigated Soils of the M.I.A., NSW
	Project Code:	IS	Site ID:	C656b	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	J. Loveday	Locality:	Approximately 20 kilometres southeast of Griffith.  
	Whitton, NSW.
	Date Desc.:	01/01/66	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	146.13333333	Runoff:	No Data
	Easting/Lat.:	-34.45	Drainage:	No Data
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Ug5.34
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark grey (10YR4/1-Moist); ; Medium clay; Very few (0 - 2 %), Calcareous, , Concretions; 
	0.1 - 0.9 m	Brown (10YR4/3-Moist); ; Medium clay; , Angular blocky; Very few (0 - 2 %), Calcareous, , 
	Concretions; 
	Morphological Notes
	Observation Notes
	GSG = Grey - brown clay.
	Site Notes
	Site a and b are no more than 10 to 20m apart

	Project Name:	Irrigated Soils of the M.I.A., NSW
	Project Code:	IS	Site ID:	C656b	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 10	7.4A	0.15A	17.8A	9.2	1.8	1	3.9D	33.7B
	10 - 20	8.6A	0.21A
	20 - 30	8.9A	0.3A	12.5E	15.2	1	3.6	0D	32.3B
	30 - 40	8.9A	0.39A
	40 - 60	9.2A	0.3A
	60 - 80	9.4A	0.27A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 10	1.24	9C	26	7	58
	10 - 20	1.35
	20 - 30	1.21B	1.36	4C	21	7	68
	30 - 40	1.47
	40 - 60	1.46
	60 - 80	1.47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 10	0.2B
	10 - 20
	20 - 30	0.21B
	30 - 40	0.22B
	40 - 60	0.23B
	60 - 80	0.23B

	Project Name:	Irrigated Soils of the M.I.A., NSW
	Project Code:	IS	Site ID:	C656b	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for 
	soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19B1	Carbonates - manometric
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B_GV_15	15 BAR Moisture g/g - Gravimetric using pressure plate
	P6_LP	Dispersion Index (Loveday and Pyle, 1973)